For 1990-2009 cars

### Removal Procedure

Notice: Mask all areas adjacent to roof to prevent paint damage

Important: If the reveal molding cracks, breaks, or is damaged in any way, replace the molding.

1. Starting at either windshield pillar, carefully pull off the reveal molding (5) from the front of the vehicle.
2. Pull off the reveal molding (3) from the rear of the vehicle.

### Installation Procedure

1. Position the reveal molding.
2. Beginning at the rear of the vehicle, press the reveal molding (3,5) into position.
3. Secure the reveal molding.