For 1990-2009 cars

### Removal Procedure

1. Raise the seat to the full up position.
2. Remove the rear air deflector (3).
3. Remove the folding armrest compartment (1).
4. Remove the nut (2) that retains the support bracket.
5. Remove the support bracket.

### Installation Procedure

1. Install the support bracket.
2. Install the nuts (2) in order to retain the bracket.
3. Install the folding armrest compartment (1).
4. Install the rear air deflector (3).