For 1990-2009 cars

# CLICKING NOISE COMING FROM THE OUTBOARD SIDE(S) OF THE SUNROO

#### SUBJECT: CLICKING NOISE COMING FROM THE OUTBOARD SIDE(S) OF THE SUNROOF (REMOVE MAGNETS)

#### MODELS: 1995 BUICK RIVIERA 1995 OLDSMOBILE AURORA

#### CONDITION:

SOME OWNERS MAY COMMENT ON A CLICKING NOISE COMING FROM THE OUTBOARD SIDE(S) OF THE SUNROOF.

#### CAUSE:

THE CLICKING NOISE IS BEING CAUSED BY THE MAGNETS ON BOTH OR EITHER SIDE OF THE SUNROOF ENGAGING AND DISENGAGING.

#### CORRECTION:

REMOVE BOTH MAGNETS BY USING THE FOLLOWING PROCEDURE:

1. OPEN SUNROOF AND SHADE.

2. POSITION YOURSELF IN THE OPENING FACING REARWARD.

3. PULL DOWN GENTLY ON REAR CORNER RADIUS OF THE HEADLINER AT SUNROOF OPENING.

4. INSERT LARGE BLADED SCREWDRIVER, WITH A LONG SHANK, BETWEEN MAGNET AND HEADLINER.

5. CAREFULLY TWIST SCREWDRIVER TO DISENGAGE MAGNET. MAGNET WILL STICK TO THE ROOF. USE SCREWDRIVER TO SLIDE MAGNET TO OPENING AND REMOVE.

6. CLOSE SUNROOF AND SHADE AND CHECK CLOSE-OUT BETWEEN SHADE AND HEADLINER.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T2550 LABOR TIME: 0.2 HR.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.