For 1990-2009 cars

### Removal Procedure

1. Disengage the assist handle end caps (2).
2. Slide the end caps toward the center of the strap.
3. Remove the 2 fasteners (1) retaining the handle assembly (3).
4. Remove the handle (3).

### Installation Procedure

1. Position the handle (3).
2. Install the 2 fasteners (1) in order to secure the handle (3).
3. Slide the end caps to the ends in order to engage the end caps (2).