For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Balance Shaft Gear Bolt | 22+70° | 16+70° | --
Balance Shaft Retainer Bolt | 30 | 22 | --
Belt Idler Pulley Bracket Bolt (VIN 1) | 50 | 37 | --
Belt Idler Pulley Bolt (VIN 1) | 30 | 22 | --
Camshaft Position Sensor Bolt | 10 | -- | 89
Camshaft Sprocket Bolt | 100+90° | 74+90° | --
Camshaft Thrust Plate Screw | 15 | 11 | --
Connecting Rod Cap Bolt | 27+50° | 20 +50° | --
Coolant Outlet Housing Bolt | 27 | 20 | --
Crankshaft Balancer Bolt | 150+76° | 111+76° | --
Crankshaft Main Bearing Cap Bolt | Refer to Procedure
Crankshaft Position Sensor Stud | 30 | 22 | --
Crankshaft Rear Main Oil Seal Housing Bolt | 15+50° | 11+50° | --
Cylinder Head "NEW" Bolt | Refer to Procedure
Drive Belt Tensioner Bolt | 50 | 37 | --
Drive Belt Tensioner Bracket Bolt (VIN 1) | 50 | 37 | --
EGR Valve Adapter Nut | 50 | 37 | --
EGR Valve Nut | 29 | 21 | --
EGR Valve Outlet Pipe Bolt/Nut (Except Upper Intake Manifold) | 29 | 21 | --
EGR Valve Wiring Harness Heat Shield Bolt/Nut | 10 | -- | 89
Engine Block Coolant Drain Plug | 18 | 13 | --
Engine Coolant Temperature Sensor | 25 | 18 | --
Engine Flywheel Bolt (New) | 15+50° | 11+50° | --
Engine Front Cover Bolt/Stud | 15+40° | 11+40° | --
Engine Lift Bracket Bolt/Nut/Stud | 30 | 22 | --
Engine Oil Gallery Plug | 30 | 22 | --
Exhaust Crossover Bolt/Stud | 20 | 15 | --
Exhaust Manifold Bolt/Stud | 30 | 22 | --
Fuel Injector Rail Assembly Nut | 10 | -- | 89
Fuel Injector Rail Stud | 25 | 18 | --
Generator Brace Bracket Bolt | 50 | 37 | --
Heated Oxygen Sensor | 42 | 31 | --
ICM Bracket Stud | 30 | 22 | --
ICM Assembly Nut | 8 | -- | 71
Lower Intake Manifold Bolt | Refer to Procedure
MAP Sensor Bracket Bolt | 30 | 22 | --
MAP Sensor Bolt | 3 | -- | 27
Oil Cooler Adapter Connector | 50 | 37 | --
Oil Filter Adapter Bolt | 30 | 22 | --
Oil Level Indicator Nut | 19 | 14 | --
Oil Pan Bolt | 14 | -- | 125
Oil Pan Drain Plug | 44 | 32 | --
Oil Pump Cover Screw | 11 | -- | 98
Oil Pump Screen Bolt | 15 | 11 | --
Power Brake Booster Heat Shield Nut | 20 | 15 | --
Side Main Cap Bolt | 15+45° | 11+45° | --
Sight Shield Bracket Nut | 30 | 22 | --
Starter Motor Heat Shield Bolt | 30 | 22 | --
Supercharger Bolt/Stud | 23 | 17 | --
Supercharger Bypass Valve Nut | 8 | -- | 71
Throttle Body Bolt/Nut | 10 | -- | 89
Throttle Body Support Bolt | 10 | -- | 89
Timing Chain Dampener Bolt | 22 | 16 | --
Upper Intake Manifold Bolts | Refer to Procedure
Valve Lifter Guide Retainer Bolt | 30 | 22 | --
Valve Rocker Arm Bolt | 15+90° | 11+90° | --
Valve Rocker Arm Cover Bolt | 10 | -- | 89
Water Pump Bolt | 15+80° | 11+80° | --
Water Pump Pulley Bolt | 13 | -- | 116