For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the seat back. Refer to Rear Seat Back Replacement in Seats.
3. Remove the sail panels. Refer to Sail Panel Replacement in Seats.
4. Remove the seat belt guide fastener and guide.
5. Remove the body lock pillar trim. Refer to Body Lock Pillar Trim Replacement .
6. Remove the coat hook cover (2).
7. Remove the fastener.
8. Pull rear coat hook (1) downward away from headliner.
9. Disconnect the electrical connector.
10. Remove the rear coat hook assembly.

### Installation Procedure

1. Connect the electrical connector.
2. Install the rear coat hook assembly (1).
3. Install the fastener.
4. Install the coat hook cover (2).
5. Install the body lock pillar trim. Refer to Body Lock Pillar Trim Replacement .
6. Install the seat belt guide and fastener.
7. Install the sail panel. Refer to Sail Panel Replacement in Seats.
8. Install the seat back. Refer to Rear Seat Back Replacement in Seats.
9. Install the seat cushion. Refer to Rear Seat Cushion Replacement in Seats.