For 1990-2009 cars

# RECOMMENDED REFRIGERANT CAPACITY (INFORMATION)

#### SUBJECT: RECOMMENDED REFRIGERANT CAPACITY (INFORMATION)

#### MODELS: 1994 BUICK LESABRE AND PARK AVENUE 1995 BUICK RIVIERA 1994 OLDSMOBILE EIGHTY EIGHT AND NINETY EIGHT 1995 OLDSMOBILE AURORA 1994 PONTIAC BONNEVILLE

SOME OF THE ABOVE VEHICLES MAY HAVE AN INCORRECT REFRIGERANT CAPACITY LABEL INDICATING THE REFRIGERANT CAPACITY IS .906 KG. (2.2 POUNDS). IT SHOULD BE NOTED THAT THE CORRECT REFRIGERANT CAPACITY OF THESE VEHICLES IS .906 KG. (2.0 POUNDS).

NO AIR CONDITIONING SERVICE IS REQUIRED. THESE VEHICLES ARE PRODUCED WITH THE CORRECT .906 KG. (2.0 POUNDS) CAPACITY CHARGE. HOWEVER, IF IT IS NECESSARY TO SERVICE THE AIR CONDITIONING SYSTEMS ON THESE VEHICLES, FOLLOW THE PROCEDURES IN SECTION 1B OF THE APPROPRIATE SERVICE MANUAL. FOR PROPER AIR CONDITIONING PERFORMANCE, THE SYSTEMS SHOULD BE CHARGED WITH NO MORE THAN .906 KG. (2.0 POUNDS).

#### NOTE: THE SERVICE AND OWNER'S MANUALS MAY ALSO HAVE AN INCORRECT REFRIGERANT CAPACITY LISTED. PLEASE MAKE REFERENCE OF THE ABOVE INFORMATION TO THESE MANUALS ALSO.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.