For 1990-2009 cars

# EXCHANGE PROGRAM - INFO. ON DLR. INSTALLED CELL. TELEPHONE

THIS BULLETIN IS BEING REVISED TO INFORM "GM OF CANADA" AND "NAES" DEALERS THAT THEY ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN

*********************************************************************

"GM OF CANADA" AND "NAES" DEALERS ARE NOT AUTHORIZED TO UTILIZE THIS SERVICE BULLETIN.

*********************************************************************

#### SUBJECT: EXCHANGE PROGRAM - INFORMATION ON DIAGNOSTICS/REPLACEMENT OF DEALER INSTALLED CELLULAR TELEPHONE

#### MODELS: 1995 BUICK RIVIERA 1995 OLDSMOBILE AURORA

CELLULAR PHONE DIAGNOSTICS/GENERAL NOTES:

THE FOLLOWING INFORMATION INCLUDES THE DEALER INSTALLED CELLULAR TELEPHONE PROGRAM THEORY OF OPERATION, SYMPTOM CHART, AND WIRING DIAGRAM.

THE SYMPTOM CHART SHOULD BE THE STARTING POINT FOR TROUBLESHOOTING THIS SYSTEM (SEE ATTACHMENT). THE WIRING DIAGRAMS ARE THERE FOR YOUR REFERENCE.

WHILE SERVICING THE DEALER INSTALLED CELLULAR TELEPHONE, IT MAY BE NECESSARY TO PLACE A CALL TO TEST THE TELEPHONE'S OPERATION. THESE PHONE CALLS SHOULD BE MADE TO A LOCAL TELEPHONE AND MUST BE BRIEF. THE OWNER SHOULD ALSO BE MADE AWARE THAT THIS MIGHT TAKE PLACE AND THERE MAY BE A SMALL CHARGE ON THEIR TELEPHONE BILL FOR THE TIME THE PHONE WAS USED. THE WAY THE SYSTEM IS SET UP, THE USER OF THE TELEPHONE PAYS FOR THE TIME THE TELEPHONE IS IN USE - WHETHER THE CALL IS AN INCOMING CALL OR AN OUTGOING CALL.

CELLULAR TELEPHONES ARE SIMILAR TO AN FM RADIO IN TERMS OF RECEPTION. THAT MEANS THE CELLULAR TELEPHONE WILL EXHIBIT THE SAME CHARACTERISTICS AS YOUR RADIO. THE DIFFERENCE OCCURS WHEN THE USER TRAVELS INTO AREAS WHERE THE CELLULAR TELEPHONE RECEPTION IS WEAK. THE TRAVELER MAY EXPERIENCE MULTIPATH INTERFERENCE WHILE TRAVELING NEAR THESE FRINGE AREAS. WHEN THE CELLULAR TELEPHONE EXPERIENCES A WEAK ENOUGH SIGNAL, IT WILL DROP THE TELEPHONE CALL. WHEN THIS HAPPENS, THE USER WILL HAVE TO RE-INITIATE THE PHONE CALL. THE PHONE WILL NOT ATTEMPT TO KEEP THE PHONE CALL CONNECTED.

THE PROGRAMMING PROCEDURES FOR THE CELLULAR TELEPHONE CAN BE FOUND IN THE USER'S MANUAL AND THE CELLULAR TELEPHONE ACTIVATION PROCEDURES CAN BE FOUND IN THE DEALER ACTIVATION GUIDE. IF YOU HAVE ANY QUESTIONS REGARDING THESE PROCEDURES, PLEASE REFER TO THESE DOCUMENTS.

THE "G" CAR CELLULAR PHONE IS DIFFERENT THAN THE PAST DE CELLULAR PHONE KITS IN THAT IT IS MORE PORTABLE AND HAS LESS EXTERIOR PARTS. THE WIRING IS MORE SIMPLIFIED THAN THOSE OF THE PAST. CHECK WIRING AND COMPONENTS DIAGRAM ON THE ATTACHED PAGE.

#### REPLACEMENT:

1. VERIFY AND DIAGNOSE THE OWNER'S CONCERN. IF THE HANDSET IS DEFECTIVE, PROCEED TO STEP 2. IF ANY OTHER PART IS DEFECTIVE, REPLACE THE PART FROM THE FOLLOWING PARTS LIST:

SERVICE PARTS AURORA RIVIERA ============= ====== =======

HAND PORTABLE PHONE 16204847 16204810 BATTERY 16206283 16206283 USER'S MANUAL 16204852 16204852 MICROPHONE 16157221 16157221 COIL CORD 16204804 16204804 CHARGER CORD 16204806 16204806 PHONE HARNESS 16204807 16204807 DOCKING CUP 16204853 16204853 SPEAKER 16157996 16157996 POWER HARNESS 16204808 16204808 AC TRANSFORMER 16207215 16207215 HARDWARE KIT 16206637 16206635 - SPLICE KIT (6) - TIE STRAPS (3) - BRACKET MOUNTING SCREWS (4) - FASTENERS (4) MOUNTING BRACKET 16204857 16204811 ANTENNA 16175583 16175583

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

2. IF THE IN-WARRANTY HANDSET IS DEFECTIVE, GATHER THE FOLLOWING INFORMATION: (IF OUT-OF-WARRANTY, SEE STEP 7)

- DEALER NAME, ADDRESS, AND DEALER CODE - OWNER'S NAME, CELL PHONE NUMBER AND DEFECTIVE HANDSET'S ESN (THIS NUMBER IS FOUND BY REMOVING THE BATTERY PACK AND LOOKING AT THE BAR CODE LABEL. THE ESN BEGINS WITH 82 OR C).

3. OBTAIN A NEW HANDSET FROM THE "G" CAR CELL PHONE SALES KIT THAT IS REQUIRED TO BE STOCKED BY EACH DEALER. THIS HANDSET WILL BE THE REPLACEMENT FOR THE OWNER'S DEFECTIVE HANDSET. A NEW HANDSET WILL BE SENT (SEE STEP 5) TO MAKE THE SALES KIT COMPLETE. THE OWNER'S BATTERY PACK FROM THE DEFECTIVE HANDSET MUST BE TRANSFERRED TO THE NEW HANDSET.

4. CONTACT THE GM ACTIVATION CENTER (1-800-422-2394) TO TRANSFER THE OWNER'S PHONE NUMBER TO THE REPLACEMENT HANDSET. YOU WILL NEED THE REPLACEMENT HANDSET'S ESN (SEE STEP 2) AND THE OWNER'S PHONE NUMBER AT THE TIME YOU CALL THE ACTIVATION CENTER. THIS PROCESS TAKES FROM 30 MINUTES TO 4 HOURS DEPENDING ON THE PHONE CARRIER. THE ACTIVATION CENTER WILL CONTACT THE DEALER WHEN THE PROCESS IS COMPLETE.

5. CALL 1-800-323-4813 (NATIONAL), 708-916-8787 (LOCAL CHICAGO), OR 708-916-8922 (FAX) TO REQUEST A REPLACEMENT HANDSET. THE REPLACEMENT WILL BE SHIPPED WITHIN 24 HOURS, SECOND DAY SHIPPING. YOU WILL BE ASKED TO PROVIDE THE INFORMATION OBTAINED IN STEP 2 ALONG WITH YOUR NAME.

6. AFTER RECEIPT OF THE REPLACEMENT HANDSET, PACK THE DEFECTIVE HANDSET USING THE BOX AND PACKING THAT THE REPLACEMENT HANDSET ARRIVED IN, ENCLOSE A COPY OF THE REPAIR ORDER FOR THE DEFECTIVE HANDSET, AND SHIP USING THE RETURN LABEL PROVIDED. USE REGULAR GROUND SHIPPING FOR THE DEFECTIVE HANDSET.

7. IF THE PHONE IS OUT-OF-WARRANTY, THE REPLACEMENT HANDSET IS PURCHASED THROUGH SERVICE PARTS OPERATION.

FIGURES: 0 ATTACHMENTS: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.