For 1990-2009 cars

### Removal Procedure

1. From the inside of the rear compartment, remove the 2 push-in retainers (2) from the high mounted stop lamp access cover (1).
2. Push upward and rotate the center brace away from the insulation.
3. Remove the screws (3) that retain the high mounted stop lamp to the rear shelf (1).
4. Remove the lamp assembly (2) by pushing the lamp rearward in order to disengage the tabs.
5. Turn the sockets in a counterclockwise direction in order to remove the sockets from the lamp assembly.
6. Remove the bulbs from the sockets.

### Installation Procedure

1. Install the bulbs to the sockets.
2. Turn the sockets in a clockwise direction in order to retain the sockets to the lamp assembly (2).
3. Install the lamp assembly (2) by pushing the lamp forward and engaging the tabs.
4. Install the screws (3).
5. Install the center brace.
6. Install the high mounted stop lamp access cover (1) and the 2 retainers (2).