For 1990-2009 cars

### Normal Vehicle Use

The maintenance instructions contained in this schedule are based on the assumption that the vehicle will be used as designed:

• | To carry passengers and cargo within the recommended limitations as indicated on the tire placard located on the edge of the driver's door.

• | On reasonable road surfaces and within legal driving limits.

• | Using unleaded gasoline of the recommended type. For information on the proper type of fuel to use refer to the Owner's Manual.

### Maintenance Schedule Intervals

The services shown in this schedule up to 166 000 km (100,000 miles) should be performed after 166 000 km (100,000 miles) at the same intervals. The services shown in this schedule to be performed at 240 000 km (150,000 miles) should be performed after 240 000 km (150,000 miles) at the same intervals.

For explanations of the maintenance inspections and services included in this maintenance schedule, refer to Explanation of Scheduled Services .

For additional maintenance inspections and services which are not included in this maintenance schedule, refer to Inspections and Other Services and Periodic Maintenance Inspection .

### Maintenance Schedule Engine Oil Change Intervals

This vehicle is equipped with an engine oil life monitor. The engine oil life monitor will indicate when to change the engine oil - usually between 5 000 km (3,000 miles) and 16 000 km (10,000 miles) since the last oil change. Under severe conditions, the CHANGE OIL message may be displayed before 5 000 km (3,000 miles).

The vehicle MUST NOT be driven more than 16 000 km (10,000 miles) or 12 months without an oil change.

The engine oil life monitor will not detect dust in the oil. If the vehicle is driven in a dusty area, be sure to change the oil every 5 000 km (3,000 miles) or sooner if the CHANGE OIL message is displayed.

### Footnotes

[Dagger] The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance item will not nullify the emission warranty or limit recall liability prior to the completion of the vehicle's useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

* This vehicle is equipped with an oil life monitor. For description and resetting information, refer to Oil Life Monitor Resetting .

#### 16 000 km (10,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

#### 32 000 km (20,000 Miles)

• | Check the engine oil life monitor. If the engine oil andthe filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

#### 48 000 km (30,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Replace the air cleaner filter.

| This is an emission control service.

• | Inspect the fuel tank, the fuel cap, and the fuel lines for damage or leaks. Inspect the fuel cap gasket for any damage. Replace any parts as needed.

| This is an emission control service. [Dagger]

#### 64 000 km (40,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

#### 80 000 km (50,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

• | Change the automatic transmission fluid and the filter if the vehicle is mainly driven under one or more of these conditions:

- | In heavy traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | For uses such as high performance operation.

If the vehicle is not used under any of these conditions, change the fluid and the filter at 166 000 km (100,000 miles).

#### 96 000 km (60,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Replace the air cleaner filter.

| This is an emission control service.

• | Inspect the fuel tank, the fuel cap, and the fuel lines for damage or leaks. Inspect the fuel cap gasket for any damage. Replace any parts as needed.

| This is an emission control service. [Dagger]

• | Inspect the accessory drive belts.

| This is an emission control service.

#### 112 000 km (70,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

#### 128 000 km (80,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

#### 144 000 km (90,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| This is an emission control service. *

• | Replace the air cleaner filter.

| This is an emission control service.

• | Inspect the fuel tank, the fuel cap, and the fuel lines for damage or leaks. Inspect the fuel cap gasket for any damage. Replace any parts as needed.

| This is an emission control service. [Dagger]

#### 160 000 km (100,000 Miles)

• | Check the engine oil life monitor. If the engine oil and the filter are changed, reset the engine oil life monitor. Refer to Oil Life Monitor Resetting .

| An emission control service. *

• | Inspect the air cleaner filter if the vehicle is driven in dusty conditions. Replace the filter if necessary.

| This is an emission control service. [Dagger]

• | Replace the spark plugs.

| This is an emission control service.

• | Inspect the spark plug wires.

| This is an emission control service.

• | Change the automatic transmission fluid and the filter if the vehicle is mainly driven under one or more of these conditions:

- | In heavy traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | For uses such as high performance operation.

If the vehicle has not been used under any of the severe conditions listed or has not had the automatic transmission fluid and the filter changed, change both the fluid and the filter.

#### 240 000 km (150,000 Miles)

Drain, flush, and refill the cooling system (or every 60 months since the last cooling system service, whichever occurs first). For information on the proper coolant to use, refer to Fluid and Lubricant Recommendations .