For 1990-2009 cars

## Power Steering Pump Pulley Replacement Buick

### Removal Procedure

#### Tools Required

J 25034-C Pulley Remover

1. Remove the pump drive belts.
2. Remove the pump from the engine. Refer to Power Steering Pump Replacement .
3. Using the J 25034-C , remove the pulley from the pump.

### Installation Procedure

#### Tools Required

J 25033-C Pulley Installer

1. Using the J 25033-C , install the pulley onto the pump.
2. Set the axial tolerance of the pulley on the pump shaft at -0.25-0.25 mm (-0.010-0.010 in).
3. Install the pump to the engine. Refer to Power Steering Pump Replacement .
4. Install the pump drive belt.
5. Bleed the power steering system. Refer to Power Steering System Bleeding .
6. Inspect the system for leaks.

## Power Steering Pump Pulley Replacement Oldsmobile

### Removal Procedure

#### Tools Required

J 38825 Pulley Remover

1. Remove the pump drive belts.
2. Remove the pump from the engine. Refer to Power Steering Pump Replacement .
3. Using the J 38825 , remove the pulley from the pump.

### Installation Procedure

#### Tools Required

J 25033-C Pulley Installer

1. Using the J 25033-C , install the pulley onto the pump.
2. Set the axial tolerance of the pulley on the pump shaft at -0.25-0.25 mm (-0.010-0.010 in).
3. Install the pump to the engine. Refer to Power Steering Pump Replacement .
4. Install the pump drive belt.
5. Bleed the power steering system. Refer to Power Steering System Bleeding .
6. Inspect the system for leaks.