For 1990-2009 cars

## Steering Column Lock Cylinder Set - Disassemble - Off Vehicle Olds

### Disassembly Procedure

1. Remove the upper tilt head components assembly. Refer to Steering Column Tilt Head Housing - Disassemble - Off Vehicle .
2. Remove 2 tapping screws (1).
3. Remove the wire protector (8).
4. Remove the lock bolt support bracket (2).
5. Remove the lock bolt assembly (3).
6. Remove the ignition lock actuator assembly (4).
7. Remove the steering column pass key lock cylinder set (5).
8. Remove the lock preload spring (7).
9. Remove the closeout knob (6).

## Steering Column Lock Cylinder Set - Disassemble - Off Vehicle Buick

### Disassembly Procedure

1. Remove the upper tilt head components assembly. Refer to Steering Column Tilt Head Housing - Disassemble - Off Vehicle .
2. Remove 2 tapping screws (1).
3. Remove the wire protector (8).
4. Remove the lock bolt support bracket (2).
5. Remove the lock bolt assembly (3).
6. Remove the ignition lock actuator assembly (4).
7. Remove the steering column pass key lock cylinder set (5).
8. Remove the lock preload spring (7).
9. Remove the closeout knob (6).