For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Instrument Cluster
2 | Was the battery disconnected? | -- | Go to Step 4 | Go to Step 3
3 | Inspect the following terminals for proper terminal contact:

• | Power feed terminal D15

• | Ground terminal C12

• | Ground terminal D12

• | Ground terminal B10

Are the connections OK?

--

Go to Step 6

Go to Step 5

4 |

1. Connect the scan tool.
2. Clear the codes.
3. Scan for codes.

Is DTC B0073 present?

--

Go to Step 3

Go to Instrument Cluster System Check

5 | Repair the poor terminal connection. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
6 | Replace the instrument cluster. Refer to Instrument Cluster Replacement . Is the repair complete? | -- | Go to Instrument Cluster System Check | --