For 1990-2009 cars

# BRUISES/WHITE STRESS MARKS REPAIR OF PLASTIC PARTS

IF POLYPROPYLENE PARTS ARE FOUND TO HAVE BRUISES OR WHITE STRESS MARKS, THE FOLLOWING PROCEDURE SHOULD BE USED BEFORE ANY ATTEMPT IS MADE TO PAINT OR REPLACE THE PART. USING A 400C (750F) HEAT GUN AND A SLOW CIRCULAR HAND MOTION, APPLY HEAT TO THE AFFECTED AREA. BRUISES OR WHITE STRESS MARKS WILL GRADUALLY DISAPPEAR. CARE MUST BE EXERCISED SO PLASTIC DOES NOT LOSE ITS PATTERN OR GRAIN FROM USE OF EXCESSIVE HEAT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.