For 1990-2009 cars

### Removal Procedure

1. Remove the EVAP canister retaining bolt.
2. Remove the hoses from the canister.
3. Mark the hoses for installation on the canister.
4. Remove the rear left exhaust retainer and hanger.
5. Remove the EVAP canister assembly from vehicle.
6. Remove the cover and canister by releasing 3 lock tabs.
7. Remove the EVAP canister.

### Installation Procedure

1. Install the EVAP canister into the cover.
2. Install the EVAP canister assembly into the vehicle.
3. Install the EVAP canister retaining bolt.
4. Connect the hoses to the canister.
5. Install the rear left exhaust retainer and hanger.