For 1990-2009 cars

## Compressor Control Switches Removal HT6/HD6

#### Tools Required

• | J 34992 Compressor Holding Fixture

• | J 5403 Snap Ring Pliers

• | J 9553-01 O-Ring Remover

1. Install the compressor into the J 34992 .
2. Remove the switch retaining ring using the J 5403 .
3. Remove the switch (2) from the compressor.
4. Remove the old O-ring seal from the switch cavity using the J 9553-01 .
5. Inspect the switch cavity and the O-ring groove in the rear head for dirt or foreign material. Clean the components as necessary.