For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the entire Exterior Lights System Check? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Disconnect the turn/hazard switch assembly connector C202.
2. Connect a fused jumper between the turn/hazard switch assembly connector C202 cavity A8 (TAN) and cavity A9 (ORN)
3. Set the headlamp switch to the PARK position.

Does the RH cornering lamp turn on?

--

Go to Step 3

Go to Step 4

3 | Replace the turn/hazard switch assembly. Refer to Turn Signal and Multifunction Switch Assembly - Disassemble - Off Vehicle in Steering Wheel and Column - Tilt. Is the repair complete? | -- | Go to Exterior Lights System Check | --
4 | Inspect CKT 58 (ORN) for an open or short to ground. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 58 OK? | -- | Go to Step 5 | Go to Step 7
5 | Inspect CKT 1350 (BLK) for an open between S115 and the RH cornering lamp. Refer to Testing for Continuity in Wiring Systems. Is CKT 1350 OK? | -- | Go to Step 6 | Go to Step 7
6 | Replace the RH cornering lamp. Refer to Cornering Lamp Replacement . Is the repair complete? | -- | Go to Exterior Lights System Check | --
7 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --