For 1990-2009 cars

## Power Mirrors Inoperative in Left/Right Direction - Right Side Without Memory

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Mirrors System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 |

1. Disconnect the RH outside rear view mirror connector.
2. Disconnect the outside mirror switch connector.
3. Connect the digital multimeter (DMM) between the mirror switch connector terminal E and the RH outside rear view mirror connector terminal B.

Does the resistance measure within the specified range?

0-5 ohms

Go to Step 3

Go to Step 4

3 | Connect a DMM between the outside mirror switch connector terminal M and the RH outside rear view mirror connector terminal A. Does the resistance measure within the specified range? | 0-5 ohms | Go to Step 5 | Go to Step 6
4 | Repair a faulty connection or an open in CKT 881 (RED/WHT). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
5 | Connect a DMM between the outside mirror switch connector terminal C and the RH outside rear view mirror connector terminal C. Does the resistance measure within the specified range? | 0-5 ohms | Go to Step 7 | Go to Step 8
6 | Repair a faulty connection or an open in CKT 82 (LT BLU). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
7 | Connect a DMM between the outside mirror switch connector terminal S and the RH outside rear view mirror connector terminal D. Does the resistance measure within the specified range? | 0-5 ohms | Go to Step 9 | Go to Step 10
8 | Repair a faulty connection or open in CKT 889 (PPL/WHT). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
9 |

1. Move the mirror select switch to the right position.
2. Connect a DMM between the RH outside rear view mirror connector terminal C and ground.
3. Position the mirror switch to the down position.

Does the voltage measure within the specified range?

10-15 V

Go to Step 11

Go to Step 12

10 | Repair a faulty connection or an open in CKT 88 (YEL). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
11 |

1. Connect a DMM between the RH outside rear view mirror connector terminal B and ground.
2. Position the mirror switch to the right position.

Does the voltage measure within the specified range?

10-15 V

Go to Step 15

Go to Step 12

12 | Test the mirror switch connector terminal contact. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Is there proper terminal contact? | -- | Go to Step 14 | Go to Step 13
13 | Repair the improper terminal contact. Refer to Connector Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
14 | Replace the outside mirror switch. Refer to Power Mirror Switch Replacement . Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
15 | Test the RH outside rear view mirror connector terminal contact. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Is there proper terminal contact? | -- | Go to Step 17 | Go to Step 16
16 | Repair the improper terminal contact. Refer to Connector Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Outside Mirrors System Check | --
17 | Replace the RH outside rear view mirror. Refer to Power Mirror Replacement . Did you complete the repair? | -- | Go to Outside Mirrors System Check | --