For 1990-2009 cars

## Power Seat Switch Replacement Buick

### Removal Procedure

1. Disconnect the fasteners.
2. Disconnect the electrical connectors (2).
3. Remove the seat switch (1).

### Installation Procedure

1. Connect the electrical connectors (2).
2. Install the seat switch (1).
3. Install the fasteners.

## Power Seat Switch Replacement Oldsmobile

### Removal Procedure

1. Remove the inner door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the trim panel insert. Refer to Power Accessory Switch Panel Replacement .
3. Disconnect the electrical connector.
4. Remove the seat switch (2).

### Installation Procedure

1. Install the power seat switch (2).
2. Connect the electrical connector.
3. Install the trim panel insert. Refer to Power Accessory Switch Panel Replacement .
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .