For 1990-2009 cars

### Removal Procedure

1. Remove the left side sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.
2. Disconnect the electrical connector from the module.
3. Remove the body control module (1).

### Installation Procedure

1. Install the body control module (1).
2. Connect the electrical connector.
3. Install the sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.