For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 | Using the instrument panel-mounted rear compartment release switch, verify the rear compartment lid release function. Does the rear compartment lid release system operate? | -- | Go to Step 3 | Go to Rear Compartment Lid Release System Check in Body Rear End
3 | Is the rear compartment release inoperative from both transmitters? | -- | Go to Step 4 | Go to Step 7
4 | Inspect CKT 1344 (LT BLU) for an open between the remote function actuator module and the rear compartment lid release relay. Was an open found? | -- | Go to Step 5 | Go to Step 6
5 | Repair the open in CKT 1344 (LT BLU) . Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --
6 | Replace the RKE module. Refer to Remote Control Door Lock Receiver Replacement . Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --
7 |

1. Replace the transmitter. Refer to Transmitter Programming .
2. Reprogram the transmitter.

Is the repair complete?

--

Go to Remote Keyless Entry System Check

--