For 1990-2009 cars

## Power Door Locks Inoperative - One Motor Except Left Front

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Door Locks System Check? | -- | Go to Step 2 | Go to Power Door Locks System Check
2 |

1. Use a digital multimeter (DMM) in order to backprobe the inoperative door lock actuator connector C2 between terminal A and ground.
2. Press the door lock switch to the UNLOCK position.

Does the voltage measure within the specified range?

10-15 V

Go to Step 4

Go to Step 3

3 | Repair an open in CKT 294 (TAN). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Power Door Locks System Check | --
4 |

1. Use a DMM in order to backprobe the inoperative door lock actuator between connector C2 terminal B and ground.
2. Press the door lock switch to the LOCK position.

Does the voltage measure within the specified range?

10-15 V

Go to Step 6

Go to Step 5

5 | Repair an open in CKT 295 (GRY). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Power Door Locks System Check | --
6 | Replace the inoperative door lock actuator. Refer to one of the following procedures:

• | Door Lock Actuator Replacement

• | Rear Side Door Lock Actuator Replacement

Did you complete the repair?

--

Go to Power Door Locks System Check

--

## Power Door Locks Inoperative - One Motor Left Front

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Door Locks System Check? | -- | Go to Step 2 | Go to Power Door Locks System Check
2 |

1. Use a digital multimeter (DMM) in order to backprobe the inoperative left front door lock actuator connector between terminal A and ground.
2. Press the door lock/window switch to the UNLOCK position.

Does the voltage measure within the specified range?

10-15 V

Go to Step 4

Go to Step 3

3 | Repair an open in CKT 694 (TAN). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Power Door Locks System Check | --
4 |

1. Use a DMM in order to backprobe the inoperative LH front door lock actuator between the connector terminal B and ground.
2. Press the door lock/window switch to the LOCK position.

Does the voltage measure within the specified range?

10-15 V

Go to Step 6

Go to Step 5

5 | Repair an open in CKT 295 (GRY). Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Power Door Locks System Check | --
6 | Replace the inoperative LH front door lock actuator. Refer to Door Lock Actuator Replacement . Did you complete the repair? | -- | Go to Power Door Locks System Check | --