For 1990-2009 cars

# BODY AND FRAME MOUNT TORQUE SPECIFICATIONS

THE TORQUE SPECIFICATIONS FOR THESE MOUNTS WERE NOT LISTED IN THE 1980 SERVICE MANUAL HOWEVER, THEY WILL BE LISTED IN THE 1981 SERVICE MANUAL. WHEN USING THE FOLLOWING CHART, YOUR ATTENTION SHOULD BE DIRECTED TO THE GREATER TORQUE SPECIFICATION ON G.M.A.D. PRODUCED CUTLASS, 88 AND TORONADO CARS. THIS IS DUE TO THE G.M.A.D. PLANTS USING SELF TAPPING BOLTS. 1980-81 TORQUE SPECIFICATIONS BODY MOUNTS CUTLASS ALL POSITIONS-PLANT CODE "M"..... N.M 36 FT.LBS. 27 ALL POSITIONS-EXC.PLANT CODE "M".. N.M 70 FT.LBS. 52 88-98 ALL POSITIONS-PLANT CODE "M"..... N.M 36 FT.LBS. 27 ALL POSITIONS-EXC. PLANT CODE "M".. N.M 70 FT.LS. 52 TORONADO ALL POSITIONS................. N.M 36 FT.LBS. 27 FRAME BRACES CUTLASS BRACE TO FRAME............... N.M 85 FT.LBS. 63 BRACE TO CROSSMEMBER.......... N.M 33 FT.LBS. 24 88-98 ALL BRACES (BOLTS).............. N.M 85 FT.LBS. 63

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.