For 1990-2009 cars

## Electronic Traction Control Switch Replacement Buick

### Removal Procedure

1. Remove the instrument panel (IP) cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Turn the traction control/trip odometer reset switch assembly (1) counter clockwise in order to disengage the switch.
3. Remove the switch.

### Installation Procedure

1. Align the retainers on the traction control/trip odometer reset switch (1) to the instrument panel (IP) cluster trim plate.
2. Turn the switch assembly clockwise in order to fasten the switch.
3. Install the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .

## Electronic Traction Control Switch Replacement Oldsmobile

### Removal Procedure

1. Remove the shifter trim plate. Refer to Front Floor Console Trim Plate Replacement .
2. Use a flat-bladed tool in order to disengage the retainers that fasten the traction control switch (1).
3. Remove the switch (1).

### Installation Procedure

1. Align the traction control switch (1) to the shifter trim plate.

Push inward in order to fasten the switch.

2. Install the shifter trim plate. Refer to Front Floor Console Trim Plate Replacement .