For 1990-2009 cars

### Assembly Procedure

Tools Required
J 23653-SIR Lock Plate Compressor

Important: Align the block tooth on the race and upper shaft assembly with the 12 o'clock position.

1. Install the inner race (1).
2. Install the upper bearing inner race seat (2).
3. Install the upper bearing spring (3).
4. Install the turn signal cancel cam assembly (4). Lubricate with synthetic grease.
5. Install the shaft lock (5).
6. Use the J 23653-SIR in order to install the bearing retainer.
7. Install the SIR coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Assemble - Off Vehicle .