For 1990-2009 cars

### Removal Procedure

1. Lower the headliner in order to access the drain hose connections. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Remove the clamp and the drain hose from the drain spout.
3. Remove the interior moldings in order to access the drain hose retaining clips. Refer to Windshield Pillar Garnish Molding Replacement and to Sail Panel Replacement in Interior Trim.
4. Remove the tape from the drain hose.
5. Remove the front drain hose (1) from the retaining clips.
6. Remove the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement in Body Rear End.

Remove the rear upper drain hose (1) from the retaining clips.

7. Remove the rear lower drain hose from the retaining clips.

### Installation Procedure

1. Clip the rear lower drain hose into position.
2. Install the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement in Body Rear End.
3. Clip the rear upper drain hose (1) into position.
4. Clip the front drain hose (1) into position.
5. Install the interior moldings. Refer to Windshield Pillar Garnish Molding Replacement and to Sail Panel Replacement in Interior Trim.

Important: When installing the drain hose clamps, position the clamps in order to maintain clearance between the clamps and the headliner.

6. Install the drain hose to the drain spout.

Notice: Use care when removing and installing the headliner. If reusing the headliner lay the headliner down flat on a clean surface. Excessive bending will damage the headliner.

7. Install the headliner to the roof. Refer to Headlining Trim Panel Replacement in Interior Trim.