For 1990-2009 cars

## Radio Replacement Buick

### Removal Procedure

1. Remove the instrument cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement in Instrument Panel, Gauges and Console.
2. Remove the fasteners (1) that retain the radio to the instrument panel.
3. Disconnect the electrical connector (3).
4. Disconnect the antenna lead (4) from the radio.
5. Remove the radio (2).

### Installation Procedure

1. Install the radio (2).
2. Connect the electrical connector (3) .
3. Connect the antenna lead (4) to the radio.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the fasteners (1) in order to retain the radio to the instrument panel.

Tighten
Tighten the fasteners to 1.9 N·m (17 lb in).

5. Install the instrument cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement in Instrument Panel, Gauges and Console.

## Radio Replacement Oldsmobile

### Removal Procedure

1. Remove the center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.
2. Remove the fasteners (3) that retain the radio to the instrument panel.
3. Remove the radio (2) from the instrument panel assembly.
4. Disconnect the electrical connectors (1).
5. Disconnect the antenna lead (6) from the radio.

### Installation Procedure

1. Connect the electrical connectors (1).
2. Connect the antenna lead (6) to the radio.
3. Install the radio (2) to the instrument panel assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the fasteners (3) in order to retain the radio to the instrument panel.

Tighten
Tighten the fasteners to 1.9 N·m (17 lb in).

5. Install the center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.