For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Nut at the Solenoid | 8 N·m | 71 lb in
Battery Cable to Battery Post | 15 N·m | 11 lb ft
Battery Cable to Generator Output Stud | 20 N·m | 15 lb ft
Battery Cable to Generator Output Stud (L47) | 15 N·m | 11 lb ft
Battery Cable to Starter | 10 N·m | 88 lb in
Battery Hold Down Retainer Bolt | 18 N·m | 13 lb ft
Engine Ground Cable | 30 N·m | 22 lb ft
Flywheel Inspection Cover Bolts | 15 N·m | 11 lb ft
Generator Front Studs | 38 N·m | 28 lb ft
Generator Mounting Bolt ( L67) | 50 N·m | 37 lb ft
Generator Mounting Bolt (L47) | 47 N·m | 36 lb ft
Generator Output Wire ( L47, L67) | 20 N·m | 15 lb ft
Negative Battery Cable Bolt at the Battery | 15 N·m | 11 lb ft
Positive Battery Cable Bolt at the Battery | 15 N·m | 11 lb ft
Positive Booster Cable Bolt at the Multifuse Relay Center | 20 N·m | 15 lb ft
Solenoid Battery Terminal Nut | 16 N·m | 12 lb ft
Solenoid Screw | 6.5 N·m | 60 lb in
Solenoid S Terminal Nut | 3 N·m | 26 lb in
Spark Plug | 15 N·m | 11 lb ft
Starter Motor Mounting Bolt | 30 N·m | 22 lb ft