For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the negative battery cable. Refer to Battery Cable in Engine Electrical.
3. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Body and Accessories.
4. Release the tabs from the rear relay electrical center (1) cover.
5. Remove the fuel pump relay from the rear relay electrical center.

### Installation Procedure

1. Install the fuel pump relay into the rear relay electrical center.
2. Install the rear relay electrical center (1) cover.
3. Turn the ignition OFF.
4. Install the negative battery cable. Refer to Battery Cable in Engine Electrical.
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Body and Accessories.