For 1990-2009 cars

## Outside Mirrors System Check With Memory

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Set the mirror switch to left.
2. Briefly press each of the following mirror switches:

• | LEFT

• | RIGHT

• | UP

• | DOWN

The left outside rear view power mirror moves in the selected direction.

• | Power Mirrors Inoperative

• | Power Mirrors Inoperative in Left/Right Direction - Left Side

• | Power Mirrors Inoperative in Up/Down Direction - One

2 |

1. Set the mirror switch to right.
2. Briefly press each of the following mirror switches:

• | LEFT

• | RIGHT

• | UP

• | DOWN

The right outside rear view power mirror moves in the selected direction.

• | Power Mirrors Inoperative

• | Power Mirrors Inoperative in Up/Down Direction - One

• | Power Mirrors Inoperative in Up/Down Direction - One

3 | Momentarily press the DRIVER-1 switch. |

• | The following components move to the DRIVER-1 programmed settings:

• | The seat

• | Both of the outside rear view power mirrors

• | A single beep is heard.

• | Power Mirrors Inoperative

• | Power Mirrors - Memory Functions Inoperative

• | Power Mirrors - Memory Functions Inoperative

• | Power Mirrors - Memory Inoperative in One Direction

4 | Momentarily press the DRIVER-2 switch. |

• | The following components move to the DRIVER-2 programmed settings:

• | The seat

• | Both of the outside rear view power mirrors

• | A single beep is heard.

• | Power Mirrors Inoperative

• | Power Mirrors - Memory Functions Inoperative

• | Power Mirrors - Memory Functions Inoperative

• | Power Mirrors - Memory Inoperative in One Direction

5 |

1. Set the ignition switch to RUN.
2. Set the shift select to REVERSE.

The right outside rear view power mirror tilts down 5 degrees or to the end of the travel.

Parallel Park Mode Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.

## Outside Mirrors System Check Without Memory

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Put the power mirror switch in the left position.
2. Move the power mirror switch up and down.

The left outside rear view mirror moves smoothly upward and downward.

• | Power Mirrors Inoperative in Up/Down Direction - One

• | Power Mirrors Inoperative

2 | Move the power mirror switch left and right. | The left outside rear view mirror moves smoothly to the left and to the right. |

• | Power Mirrors Inoperative in Left/Right Direction - Left Side

• | Power Mirrors Inoperative

• | Power Mirrors Inoperative in Left/Right Direction - One

3 |

1. Put the power mirror switch in the right position.
2. Move the power mirror switch up and down.

The right outside rear view power mirror moves smoothly upward and downward.

• | Power Mirrors Inoperative in Up/Down Direction - One

• | Power Mirrors Inoperative

4 | Move the power mirror switch left and right. | The right outside rear view power mirror moves smoothly to the left and to the right. |

• | Power Mirrors Inoperative in Left/Right Direction - Right Side

• | Power Mirrors Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.