For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly.
2. Remove the BPMV reservoir connector.
3. Remove the clamp on the reservoir hose to the BPMV connector.
4. Obtain a 15.5 mm (5/8 in) plug in order to be used in the next step.
5. Remove the reservoir hose from the BPMV reservoir.
6. Remove the BPMV reservoir by carefully prying.
7. Remove the BPMV reservoir seals.

Note the seal orientation.

### Installation Procedure

1. Lubricate the new seals using the clean brake fluid.

Install the new seals to the BPMV.

2. Clean the reservoir and the ports with denatured alcohol.
3. Install the BPMV reservoir.
4. Install the reservoir hose to the BPMV reservoir.
5. Connect the clamp on the reservoir hose to the BPMV reservoir.
6. Install the BPMV reservoir connector.
7. Fill the brake fluid reservoir. Refer to Master Cylinder Reservoir Filling in Hydraulic Brakes.
8. Bleed the brake system. Refer to Hydraulic Brake System Bleeding in Hydraulic Brakes.
9. Clean the brake fluid from the BPMV area in order to prevent damage to the vehicle components.