For 1990-2009 cars

1. Disassemble the servo piston return spring (22) from the forward band servo assembly.
2. Remove the servo piston oil seal ring (18) from the servo piston (16).
3. Using a small screwdriver, remove the servo pin retaining ring (15) from the servo piston apply pin (21).
4. Disassemble the servo piston (16), the servo piston cushion spring (19), the servo cushion spring retainer (20) and the servo piston apply pin (21).