For 1990-2009 cars

## Front Floor Console Compartment Replacement Buick

### Removal Procedure

1. Remove the console assembly. Refer to Console Replacement .
2. Remove the console accessory housing. Refer to Console Rear Trim Plate Replacement .
3. Remove the console lower air duct fasteners (2).
4. Disengage the lower air duct from the upper air duct.

Remove the lower air duct from the console.

5. Remove the upper air duct fasteners (1).
6. Remove the upper air duct from the console.
7. Remove the console compartment fasteners (1).
8. Carefully spread the console apart.
9. Remove the console compartment.

### Installation Procedure

1. Carefully spread the console apart.
2. Install the console compartment.
3. Install the compartment fasteners (1).
4. Install the upper air duct to the console.
5. Install the upper air duct fasteners (1).
6. Install the lower air duct to the upper air duct.
7. Install the lower air duct fasteners (2).
8. Install the console accessory housing. Refer to Console Rear Trim Plate Replacement .
9. Install the console assembly. Refer to Console Replacement .

## Front Floor Console Compartment Replacement Oldsmobile

### Removal Procedure

1. Remove the fasteners (1) from the storage bin.
2. Pull upward the storage bin partially out of the console.
3. Disconnect the electrical connector (1).
4. Remove the storage bin lamp (2).
5. Remove the storage bin.

### Installation Procedure

1. Partially install the storage bin.
2. Connect the electrical connector (1).
3. Install the storage bin lamp (2).
4. Install the storage bin into the console.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the storage bin fasteners (1).

Tighten
Tighten the fasteners to 1.3 N·m (15 lb in).