For 1990-2009 cars

(1) | Refrigerant Vapor Inlet
(2) | Inlet
(3) | Baffle
(4) | Internal Tube
(5) | Desiccant Bag
(6) | Filter
(7) | Oil Bleed Hole Location--In the Tube
(8) | Outlet

The sealed accumulator is connected to the evaporator outlet pipe. The accumulator stores the refrigerant (vapor and liquid) and the oil from the evaporator. A desiccant at the accumulator bottom dries any moisture in the system. An oil bleed hole at the accumulator outlet pipe end provides the oil return path to the compressor. The accumulator is not serviceable and should only be replaced when leaking due to the following conditions:

• | Perforation

• | A damaged sealing area

• | Damaged fastener threads

• | Outside air has entered the system for extended periods of time