For 1990-2009 cars

# Warranty Admin. - January, 2000 Labor Time Guide Updates

Subject: | January, 2000 Labor Time Guide Updates

Models: | 1994-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C/K-New Body Style--Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PAN AND/OR GASKET, OIL - REPLACE

- PART GP: 1.426

- NOTE: Applies to Engine Code W

R

J1000

C TRUCK |  |  | -- | -- | -- | -- | -- | 1.2 | 1.2
K TRUCK |  |  | -- | -- | -- | -- | -- | 2.1 | 2.1
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
ENGINE ASSEMBLY - REPLACE

- PART GP: 0.033

- NOTE: Applies to Engine Code W

R

J1880

MANUAL TRANS |  |  | -- | -- | -- | -- | -- | 5.9 | 5.9
AUTO TRANS |  |  | -- | -- | -- | -- | -- | 6.2 | 6.2
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
2-4 BAND AND INPUT CARRIER ASSEMBLY - R&R OR REPLACE

- NOTE: No Change to "INCs" or "NOTE"

2-4 BAND |  | K7271 |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 5.6 | 5.6
K TRUCK | R |  | -- | -- | -- | -- | -- | 6.0 | 6.0
INPUT CARRIER ASSEMBLY |  | K7272 |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 5.7 | 5.7
K TRUCK | R |  | -- | -- | -- | -- | -- | 6.2 | 6.2
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 |  |  |  |  |  |  |
PICKUP |  |  | -- | -- | -- | -- | -- | 1.2 | 1.2
YUKON/TAHOE |  |  | -- | -- | -- | -- | -- | -- | 1.4
SUBURBAN/YUKON XL |  |  | -- | -- | -- | -- | -- | -- | 1.4
No Change to "ADD" Condition A, B, or C |  |  |  |  |  |  |  |  |
ADD:

- D- To Install Running Boards (BVE)

Suburban/Yukon XL | R |  | -- | -- | -- | -- | -- | -- | 2.0
Yukon/Tahoe | R |  | -- | -- | -- | -- | -- | -- | 2.0
*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
98 | 99 | 00 | 01
YEAR VIN CODE
W | X | Y | 1
CORE, EVAPORATOR - REPLACE

- PART GP: 9.210

D3320

OLDSMOBILE | R |  | 4.9 | 4.9 | -- | 3.3
BUICK |  |  | 3.8 | 3.8 |  |
No Change to "ADD" Conditions |  |  |  |  |  |
PAN AND/OR GASKET, OIL - REPLACE | R | J1000 | 7.2 | 7.2 | -- | 6.2
NOTE: For check and adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column | N |  |  |  |  |
NOTE: Applies to Engine Code C |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - G Van Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96-F | 96-1 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | T | V | W | X | Y
TRACK ASSEMBLY, SLIDING DOOR - REPLACE |  |  |  |  |  |  |  |  |  |
UPPER |  | B5025 | -- | -- | -- | 1.1 | 1.1 | 1.1 | 1.1 | 1.1
CENTER | R | B5026 | -- | -- | -- | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
ADD:

- A-W/Door Trim

R

--

--

--

0.4

0.4

0.4

0.4

0.4

LOWER |  | B5027 | -- | -- | -- | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MOLDING, FRONT DOOR - R&R OR REPLACE

- No Change to "PART GP" or "INC"

RIGHT |  |  |  |  |  |  |  |  |
LOWER |  | B7863 | 0.3 | 0.3 | 0.3 | 0.3 | 0.2 | 0.2 | 0.2
SIDE |  | B7866 | 0.5 | 0.5 | 0.5 | 0.5 | 0.3 | 0.3 | 0.3
LEFT |  |  |  |  |  |  |  |  |
LOWER |  | B7873 | 0.3 | 0.3 | 0.3 | 0.3 | 0.2 | 0.2 | 0.2
SIDE |  | B7876 | 0.5 | 0.5 | 0.5 | 0.5 | 0.3 | 0.3 | 0.3
ADD:

- A- To Color/Clear Coat

Lower (Right Or Left) | R |  | 0.6 GE | 0.6 GE | 0.6 GE | 0.6 GE | 0.4 GD | 0.4 GD | 0.4 GD
Side (Right Or Left) | R |  | 0.4 GD | 0.4 GD | 0.4 GD | 0.4 GD | 0.4 GD | 0.4 GD | 0.4 GD
*IND: N - New/R - Revised

#### LTG Update - Medium Duty Platform

OPERATION 0 | IND* | OP NUM | CAB STYLE YEAR VIN CODE
--- | --- | --- | ---
B | A/W5 | C | H
PUMP AND/OR GASKET, VACUUM- REPLACE

- NOTE: Applies to Engine Code 2, 3

N

J0240

--

--

--

SPROCKET, CAMSHAFT TIMING - REPLACE

- NOTE: Applies to Engine Code 2, 3

N

J0840

--

--

--

RELAY, GLOW PLUG (DIESEL) - REPLACE

- NOTE: Applies to Engine Code 2, 3

N

J4720

--

--

--

ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

PIPE, AIR CLEANER TO TURBO - REPLACE

- POLICY: E

- NOTE: Applies to Engine Code 2, 3

N

J5013

--

--

--

PIPE, INTAKE (TURBO TO INLET MANIFOLD) - REPLACE

- NOTE: Applies to Engine Code 2, 3

N

J5014

--

--

--

ENGINE EXHAUST BRAKE SYSTEM COMPONENTS - REPLACE

- NOTE: Applies to Engine Code 2, 3

CYL ASSY | R | J5392 | -- | 0.4 |  | --
VALVE ASSY | R | J5393 | -- | 1.2 |  | --
MAGNETIC VALVE | R | J5394 | -- | 0.3 |  | --
SWITCH ASSY, COMBINATION | R | J5395 | -- | 0.3 |  | --
SWITCH, ACCELERATOR EXHAUST BRAKE | R | J5396 | -- | 0.2 |  | --
SWITCH, CLUTCH EXHAUST BRAKE | R | J5397 | -- | 0.3 |  | --
TURBO TO INTERCOOLER INLET PIPE * BOTH

- NOTE: Applies to Engine Code 2, 3

N

J5691

--

--

--

SENSOR, FUEL INJECTION PUMP POSITION - REPLACE

- POLICY: E

- NOTE: Applies to Engine Code 2, 3

N

J5927

--

--

--

RAIL, COMMON FUEL - REPLACE

- POLICY: E

- NOTE: Applies to Engine Code 2, 3

N

J5929

--

--

--

PUMP, FUEL INJECTION (DIESEL) - REPLACE

- POLICY: E

- NOTE: Applies to Engine Code 2, 3

R

J5955

--

3.2

1.6

--

INC: Supply pump

- INC: R&R air intake duct, oil pipe and gaskets, fuel leak off, uncrate, time engine injection pump and prime fuel system

N

ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

0-.3

--

--

GEAR AND/OR ADVANCE TIMING MECHANISM, FUEL INJECTION PUMP - REPLACE

- POLICY: E

- NOTE: Applies to Engine Code 2, 3

R

J5962

--

4.3

--

--

TIMING, FUEL INJECTION PUMP (DIESEL) - ADJUST

- POLICY: E

- NOTE: Applies to Engine Code 2, 3

R

J5965

--

0.4

--

--

CUSTOMER CONCERN NOT DUPLICATED

- No Change to "NOTE"

- NOTE: Applies to Engine Code 2, 3

R

J9991

--

ST

ST

--

PRE-DELIVERY INSPECTION - FLUID ADD

- No Change to "NOTE"

POWER STEERING |  | E7000 |
REAR AXLE |  | F0010
BRAKE FLUID |  | H0010
ENGINE OIL |  | J0010 | THESE LABOR OPERATIONS HAVE BEEN DELETED FROM THE PRE-DELIVERY SECTION OF THE LABOR TIME GUIDE
ENGINE COOLANT |  | J3000 |
TRANSMISSION (MAN) |  | K2010
TRANSMISSION (AUTO) |  | K6100
*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
ENGINE ASSEMBLY- REPLACE

- PART GP: 0.033

J1880

M VAN |  |  |  |  |  |  |  |  |
ENGINE CODE W | R |  | 8.0 | 10.9 | 10.9 | 10.9 | 10.9 | 10.9 | 10.9
ENGINE CODE Z |  |  | 7.8 |  |  |  |  |  |
L VAN |  |  |  |  |  |  |  |  |
ENGINE CODE W | R |  | 9.2 | 10.9 | 10.9 | 10.9 | 10.9 | 10.9 | 10.9
ENGINE CODE Z |  |  | 9.0 |  |  |  |  |  |
ADD:

- A- With A/C

R

1.3

1.1

1.1

1.1

1.1

1.1

1.1

B- W/Running Boards | N |  | -- | -- | -- | -- | -- | 2.2 | 2.2
*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
SENSOR, OXYGEN (ENGINE CONTROL) - REPLACE

- POLICY: E

J6372

RIGHT BANK | R |  | 0.4 | 0.4 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
LEFT BANK |  |  | 0.4 | 0.4 |  |  |  |  |
BOTH BANKS |  |  | 0.4 | 0.4 |  |  |  |  |
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

R

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PRE-DELIVERY INSPECTION - BASE TIME | R | Z7000 | -- | -- | -- | -- | 1.2 | 1.2 | 1.2
*IND: N - New/R - Revised