For 1990-2009 cars

#### Tools Required

J 28585 Snap Ring Remover

1. Remove the thrust washer (691) from the differential carrier internal gear.
2. UseJ 28585 or a large screwdriver in order to remove the differential carrier internal gear snap ring (692).
3. Lift the differential carrier internal gear assembly (693) out of the case by depressing the park pawl assembly in order to clear the case.