For 1990-2009 cars

# SERVICE MANUAL UPDATE - SECTION 8C - REVISED

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8C - REVISED PROCEDURE FOR I/P UPPER TRIM PAD REMOVAL AND INSTALLATION

#### MODELS: 1995 BUICK RIVIERA

PLEASE REPLACE I/P UPPER TRIM PAD REMOVAL AND INSTALLATION PROCEDURE IN SECTION 8C OF THE SERVICE MANUAL WITH THE FOLLOWING REVISED PROCEDURE.

REMOVE OR DISCONNECT:

1. LEFT AND RIGHT WINDSHIELD GARNISH TRIM - PULL FROM TOP TO REMOVE, THERE ARE TWO RETAINERS ON BACK OF TRIM.

2. I/P UPPER TRIM PLATE, REFER TO PROCEDURE IN SECTION 8C.

3. SCREWS (4) FROM I/P UPPER TRIM PAD.

4. PULL TRIM PAD UP AND BACK TO DISENGAGE CLIPS (2) FROM RETAINERS (3).

5. ELECTRICAL CONNECTOR FROM BOTTOM LEFT SIDE OF I/P UPPER TRIM PAD.

6. I/P TRIM PAD.

INSTALL OR CONNECT:

1. ELECTRICAL CONNECTOR TO UPPER TRIM PAD.

2. UPPER TRIM PAD (1) TO I/P ASSEMBLY, INSERTING CLIPS (2) INTO RETAINERS (3). BE SURE THE I/P TRIM PANEL IS ALIGNED TO THE DOOR TRIM PANEL.

3. SCREWS (4).

4. I/P UPPER TRIM PLATE.

5. LEFT AND RIGHT WINDSHIELD GARNISH TRIM.

6. PULL DOOR OPENING PINCHWELD LACE OVER WINDSHIELD GARNISH MOLDING EDGE.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.