For 1990-2009 cars

## Turn Signal and Multifunction Switch Assembly - Assemble - Off Vehicle Olds

### Assembly Procedure

Important: The electrical contact of the turn signal and multifunction switch assembly must rest on the turn signal cancel cam assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the turn signal and multifunction switch assembly and secure by using 2 tapping screws.

Tighten
Tighten the screws to .5 N·m (5 lb in).

2. Install the turn signal and multifunction switch connector (2) to the bulk head connector (1).
3. Pop the wire harness assembly into the wire harness strap (1).
4. Install the upper and lower covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle

## Turn Signal and Multifunction Switch Assembly - Assemble - Off Vehicle Buick

### Assembly Procedure

Important: The electrical contact of the turn signal and multifunction switch assembly must rest on the turn signal cancel cam assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the turn signal and multifunction switch assembly and secure by using 2 tapping screws.

Tighten
Tighten the screws to .5 N·m (5 lb in).

2. Install the turn signal and multifunction switch connector (2) to the bulk head connector (1).
3. Pop the wire harness assembly into the wire harness strap (1).
4. Install the upper and lower covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .