For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)
--- | --- | --- | ---
1 |

1. Drive the vehicle above 40 km (25 mph).
2. Place the CRUISE switch in the ON position.
3. Press the SET button once and release the button.
4. Remove your foot from the accelerator pedal.

The vehicle maintains the set speed.

Cruise Control Inoperative

2 |

1. Press and hold the R/A switch until the vehicle speed increases by 6 to 8 km (4 to 5 mph).
2. Release the R/A switch.

1. The vehicle accelerates.
2. The vehicle maintains the new higher set speed.

Cruise Control Inoperative

3 |

1. Press and hold the SET button until the vehicle speed decreases by 6 to 8 km (4 to 5 mph).
2. Release the SET button.

Provided that the speed is above 40 km (25 mph), the following actions occur:

• | The vehicle decelerates to a new lower set speed.

• | The vehicle maintains the new lower set speed.

Cruise Control Inoperative

4 | Press the brake pedal slightly. |

1. The cruise control disengages.
2. The memory is unchanged.

Cruise Control Inoperative

5 |

1. Press the R/A switch once.
2. Release the R/A switch.

1. The vehicle accelerates to the previously set speed.
2. The vehicle maintains the previously set speed.

Cruise Control Inoperative

6 |

1. Press the R/A switch once (tap up).
2. Release the R/A switch within less than 3/4 second.

1. The vehicle speed increases by 1 mph.
2. The vehicle maintains the new set speed.

Cruise Control Inoperative

7 |

1. Press the SET button once (tap down).
2. Release the button within less than 3/8 of a second.

1. The vehicle speed decreases by 1 mph.
2. The vehicle maintains the new set speed.

Cruise Control Inoperative

8 | Press the SET button and the R/A switch at the same time. |

1. The cruise control disengages.
2. The memory is unchanged.

Cruise Control Inoperative

9 | Place the CRUISE switch in the OFF position. |

1. The cruise control disengages.
2. The set speed memory is erased.

Cruise Control Inoperative