For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Close the left front door.
2. Turn the ignition switch to the RUN position.
3. Unbuckle the driver's seat belt.

1. The fasten belts chime sounds for 4-8 seconds (slow-pulsed chime).
2. The FASTEN BELTS indicator illuminates for 70 seconds.

• | Fasten Safety Belt Chime Always On

• | Fasten Safety Belt Chime Inoperative

• | Fasten Safety Belt Indicator/Chime Inoperative

2 |

1. Turn the ignition switch to the OFF position.
2. Buckle the driver's seat belt.
3. Turn the ignition switch to the RUN position.

• | The fasten safety belt chime does not sound.

• | The FASTEN BELTS indicator illuminates for approximately 5 seconds (bulb check).

• | Fasten Safety Belt Chime Always On

• | Fasten Safety Belt Indicator/Chime Inoperative

3 |

1. Turn the ignition switch to the OFF position.
2. Leave the key in the ignition switch.
3. Open the left front door.

The key in ignition chime sounds (medium-pulsed chime).

• | Key-in-Ignition Chime Inoperative

• | Key-in-Ignition Chime On with Left Front Door Closed

4 | Remove the key from the ignition switch. | The key in ignition chime does not sound. | Key-in-Ignition Chime Always On
5 | Turn the headlamp switch to the PARK position. | The lamps on chime sounds (fast-pulsed chime). | Lights On Chime Inoperative
6 | Turn the headlamp switch to the OFF position. | The lamps on chime does not sound. | Lights On Chime On with Ignition in Run
7 |

1. Close the left front door.
2. Start the engine.
3. Turn the left or the right turn signal on.
4. Drive the vehicle for approximately 1.2 km (3/4 mile).

The turn signal on chime sounds after you drive approximately 1.2 km (3/4 mile).

Turn Signal Chime Inoperative

8 |

1. Apply the park brake.
2. Drive the vehicle for approximately 12 m (40 ft).

The park brake on chime sounds after driving approximately 12 m (40 ft).

Park Brake On Chime Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.