For 1990-2009 cars

# MIXTURE CONTROL SOLENOID ADJ. REVISION PLUNGER TRAVEL

MIXTURE CONTROL SOLENOID ADJUSTMENTS FOR THE 1981 CUTLASS, 88, 98 AND TORONADO MODELS 4 BBL. CARBURETOR IS DESCRIBED ON PAGE 6C1-30 OF THE 1981 SERVICE MANUAL. THE LAST SENTENCE UNDER ADJUSTMENTS SHOULD READ; IF NOT WITHIN 3-1/4 TO 3-3/4 TURNS, SOLENOID TRAVEL IS INCORRECT: ADJUST TO 3-1/2 TURNS FROM BOTTOM (FIG. 6C1-68). PLEASE MAKE THE ABOVE CORRECTION IN YOUR 1981 SERVICE MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.