For 1990-2009 cars

### Removal Procedure

1. Remove the trim panel. Refer to one of the following procedures:

• | Door Trim Panel Replacement

• | Front Side Door Trim Panel Replacement

• | Rear Side Door Trim Panel Replacement

2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Mark all of the in/out adjustments.
4. Loosen the adjusters. Refer to Door Window Adjustment or Rear Side Door Window Adjustment .
5. Disconnect the electrical connector.
6. Remove the motor attachment nuts.
7. Push the module fully outboard in order to allow for the removal of the motor (1).

### Installation Procedure

1. Install the motor (1).
2. Install the motor attachment nuts.
3. Connect the electrical connector.
4. Adjust the glass. Refer to Door Window Adjustment or Rear Side Door Window Adjustment .
5. Install the water deflector. Refer to Door Water Deflector Replacement .
6. Install the trim panel. Refer to one of the following procedures:

• | Door Trim Panel Replacement

• | Front Side Door Trim Panel Replacement

• | Rear Side Door Trim Panel Replacement