For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

Important: Before disconnecting the air hose from the intake air filter or the air compressor, clean the components and the surrounding area to prevent dirt and other foreign material from entering the air compressor.

2. Disconnect the intake air filter from the body rail and the air hose.
3. Slide the air compressor connector off of the connector anchor.
4. Remove three bolts and the heat shield from the air compressor bracket.
5. Disconnect the air hose from the air compressor assembly at two places.

### Installation Procedure

1. Connect the air hose to the air compressor assembly at two places.
2. Connect the intake air filter to the air hose and the body rail.
3. Install the heat shield and the harness tie with three bolts.

Tighten
Tighten three bolts to 4 N·m (35 lb in).

4. Install the air compressor connector onto the connector anchor.
5. Lower the vehicle. Refer to Lifting and Jacking the Vehicle .