For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the front air deflector retainers. Refer to Front Bumper Fascia Air Deflector Replacement in Bumpers.
3. Remove the wheelhouse retainers.
4. Disconnect the electrical connector.
5. Remove the retainers (2) from the fog lamp assembly.
6. Remove the fog lamp assembly (1).

### Installation Procedure

1. Install the fog lamp assembly (1).
2. Fasten the retainers (2) to the fog lamp assembly.
3. Connect the electrical connector.
4. Install the wheelhouse retainers.
5. Install the front air deflector retainers. Refer to Front Bumper Fascia Air Deflector Replacement in Bumpers.
6. Lower the vehicle.