For 1990-2009 cars

### Removal Procedure

1. Remove the trim panel. Refer to one of the following procedures:

• | Door Trim Panel Replacement

• | Front Side Door Trim Panel Replacement

• | Rear Side Door Trim Panel Replacement

2. Remove the push pins (2).
3. Remove the molding (1).

### Installation Procedure

1. Position the molding (1).
2. Install the push pins (2).
3. Install the trim panel. Refer to one of the following procedures:

• | Door Trim Panel Replacement

• | Front Side Door Trim Panel Replacement

• | Rear Side Door Trim Panel Replacement