For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2007-12-05: 60 Degree V6 Engine Oil Leak at Crankshaft Front Oil Seal (Use New Crankshaft Front Oil Seal Installer Tool EN-48869) (07-06-01-023)
- 2007-10-02: Engine Oil Leak at Crankshaft Rear Main Oil Seal (Install Revised Crankshaft Rear Main Oil Seal Using Revised Rear Main Seal Installer and Remover Tools) (05-06-01-019F)
- 2007-06-22: Abnormal Noise And Or Vibration While Driving - keywords accessory aftermarket axle body boom buzz case grown growl howl moan modification no OEM part prop rattle resonance shaft transmission whine (PIP3140B)
- 2007-03-01: Dexron VI Fluid Usage - keywords leak seal slip (PIP4066)
- 2007-01-05: Slight Vehicle Movement In Park At Start Up After Cold Soak - keywords 3T40 4L60 4L60E 4L65E 4L80E 4L85E 4T40E 4T45E 4T60 4T60E 4T65E 4T80E 5L40E 5L50E 6L50 6L80 6L90 6T70 6T75 AF225 AF235aisan (PIP3763A)
- 2007-01-04: Info - Guidelines for Using E2020-Wheel Alignments, E2000-Toe Adjust and E0200, E0201, E0203, E0204-Wheel Balance (01-03-10-012C)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2005-04-12: Info - Top Tether Hardware Package for Child Restraint Seats (99-09-40-004a)
- 2004-10-20: Info - Radio Telephone/Mobile Radio (Transceiver) Installation and Troubleshooting Guidelines (04-08-46-002)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 2002-02-27: Information on a New Engine Preluber Tool (02-06-01-008)
- 2001-05-08: Info - Replacement of Keys, Key Numbers and/or Security Chips (01-00-89-009)
- 2001-04-06: Info - Current CIPS Campaign Number to Previous DIvisional Campaign Number (01-00-89-008)
- 2001-03-28: Warranty Admin. - Inspection/Maintenance Labor Operations (01-00-89-007)
- 2001-03-02: Info - February, 2001 Bulletin Summary (01-00-89-006)
- 2000-10-06: Info - September, 2000 Bulletin Summary (00-00-89-024)
- 2000-09-05: Information - August, 2000 Bulletin Summary (00-00-89-022)
- 2000-07-06: Information - June, 2000 Bulletin Summary (00-00-89-016)
- 2000-05-30: Warranty Admin - ACDelco Remanufactured Transmissions (00-07-30-011)
- 1999-07-23: Info - Vehicles Equipped with a Webasto Sunroof System (99-08-67-003)
- 1999-03-31: Info - Cleaning of Upper Instrument Panel Surfac (99-08-49-006)
- 1999-03-04: Battery Insulator Replacement (99-06-03-002)
- 1999-02-26: Essential Tool J 42000 Battery Tester (99-06-03-001)
- 1998-11-16: INFO - ESSENTIAL TOOL J43435 ADJUSTER LOCKNUT (83-32-10)
- 1998-10-20: INFO - ESSENTIAL TOOL J43485 POWER STEERING BLEEDER ADAPTER (83-32-09)
- 1998-10-01: INFO - NEW WINDSHIELD AND STATIONATY GLASS URETHANE (83-15-16)
- 1998-08-20: INFO - ESSENTIAL TOOL J-43241 REMOTE KEYLESS ENTRY AND (83-90-12)
- 1998-08-14: INFO - CORRECT LABOR CODE USAGE FOR ENTERTAINMENT SYS. (84-96-01)
- 1998-08-12: WARRANTY ADMIN. - REDEFINED USE OF PARTS WARRANTY SPECIAL (80-05-03)
- 1998-06-03: INFO - NEW TOOL J-42958, REV. CHARTS AND SCHEM. FOR CRUISE (83-90-08)
- 1998-04-24: GENERAL MOTORS WARRANTY INQUIRY SYSTEM (82-05-05)
- 1998-04-21: WARRANTY ADMIN - REQ. FOR WHOLESALE AUTH. OR WARRANTY (82-05-02)
- 1998-04-02: INFO. USE OF'SURFACE CONDITIONING DISCS' (87-61-24)
- 1998-03-24: NEWS: INFO ON AVAIL OF SMOKE MACHINE TO DIAG. (80-15-15)
- 1998-03-16: WARRANTY ADMIN. - LABOR TIME GUIDE UPDATES (83-05-02)
- 1998-03-10: INFO. NEW TOOL J-41450-B RELEASED FOR CS GEN DIAG. (83-64-09)
- 1998-02-20: WARRANTY ADMIN - LABOR TIME GUIDE UPDATES (83-05-01)
- 1998-02-13: INFO. ON VIN PLATE REPLACEMENT (83-01-14)
- 1998-01-12: INFO. FRONT. SUPP. INFLAT. RESTRAINTS (SIR) ON-OFF SWITCH (73-90-23)
- 1997-12-18: WARRANTY ADMIN. - REPAIR/ REPLACE POLICIES & PROC. (72-05-13)
- 1997-12-18: WARRANTY ADMIN. - ENHANCED SUBLET REPAIR POLICY (72-05-14)
- 1997-12-16: WARR. ADMIN - LABOR TIME GUIDE UPDATES (73-05-09)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-11-28: WARRANTY ADMIN. - LABOR TIME GUIDE UPDATES (73-05-07)
- 1997-11-26: INFO. ON TECHNICAL ASSISTANCE CALL PREPARATION (73-01-10)
- 1997-11-20: CLARIFICATION OF RAIL DUST REM (A5575-A5580) (72-05-11)
- 1997-11-12: INFORMATION - PUREGUARD 2 OPERATING ALERT (73-12-13)
- 1997-11-07: INFO ON EXHAUST SYSTEM STAINLESS STEEL COMP. (70-66-03)
- 1997-11-01: WARRANTY ADMIN. - LABOR OPERATION CODE Z1241 (62-05-02A)
- 1997-10-24: WARR. ADMIN-LTG UPDATES 1989-98 PASS. CAR & TRUCK (73-05-06)
- 1997-09-01: INFO. ON ALUMINUM HEATER CORE AND/OR RADIATOR REPL. (73-62-13A)
- 1997-08-21: WARRANTY ADMIN - GUIDELINES FOR USING E0420 WHEEL (72-05-05)
- 1997-08-21: WARRANTY ADMIN- GUIDELINES FOR USING I/M 240 LABOR OP (72-05-06)
- 1997-08-12: WARRRANTY ADMIN - LABOR TIME GUIDE UPDATES (73-05-05)
- 1997-05-29: INFO ON AUTO TRANS OIL COOLER FLUSHING &FLOW CHECK PROC. (77-71-59)
- 1997-05-12: INFORMATION -TWO PART URETHANE ADHESIVE (73-10-54)
- 1997-04-17: INFO. ON A/C TOOL AND EQUIPMENT MAINTENANCE (63-12-08A)
- 1997-03-20: WARRANTY ADMINISTRATION - LABOR TIME GUIDE UPDATES (73-05-03)
- 1997-02-20: WARRANTY ADMINISTRATION LABOR TIME GUIDE UPDATES (73-05-02)
- 1997-02-07: SERVICE ISSUES FOR VEHICLES WITH R12 OR R134A A/C SYSTEMS (73-12-04)
- 1997-01-31: INFO. NEW BODY SEALER TAPE FOR COLLISION REPAIRS (73-10-49)
- 1997-01-24: WARRANTY ADMINISTRATION - LABOR TIME GUIDE UPDATES (73-05-01)
- 1997-01-13: INFO. ON COMPACT DISC PLAYERS- PROCEDURES (64-96-01)
- 1997-01-07: WARRANTY ADMIN. - LABOR TIME GUIDE UPDATES (63-05-07)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1996-11-21: WARRANTY ADMIN. - LABOR TIME GUIDE UPDATES (63-05-06)
- 1996-11-15: INFO. REFERENCE CHART FOR A/C COMPRESSOR SEAL WASHERS (63-12-15)
- 1996-10-15: INFO. ON THE GENERAL MOTORS KEY CODE VOICE RESPONSE SYSTEM (61-01-11)
- 1996-10-02: WARRANTY ADMIN. - LABOR TIME GUIDE UPDATES 1989 -1997 (63-05-04)
- 1996-10-01: PROCEDURE TO HANDLE CUSTOMER RADIO CONCERNS (68-96-01A)
- 1996-09-01: ACDELCO SERVICE CENTER LOC. FOR ODOMETER/SPEEDOMETER (66-83-04A)
- 1996-08-14: WARRANTY ADMIN. - LABOR TIME GUIDE ' REQUEST FOR REVIEW ' (63-05-03)
- 1996-06-05: WARRANTY ADMIN. - GOODWRENCH SERVICE PLUS LIFETIME SERVICE (68-05-03)
- 1996-05-10: INFO. ON SERVICE ISSUES FOR VEHICLES WITH R12 OR R134A (63-12-09)
- 1996-05-07: INFORMATION ON CAMPAIGN SYSTEM COMMONIZATION (62-07-01)
- 1996-05-06: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (63-65-32)
- 1996-05-01: AC DELCO LOCATOR SVCS FOR DELCO ELECTRONICS EXCHANGE (58-83-02B)
- 1996-05-01: WARRANTY ADMINISTRATION TIRE REPLACEMENTS (60-05-01A)
- 1996-04-15: INFO. ON HEADLAMP LENS DISTORTION (63-81-11)
- 1996-02-02: INFORMATION ON UPDATED BATTERY REPLACEMENT CATALOG NUMBERS (63-64-01)
- 1996-01-04: TECHNICAL ASSISTANCE PRE-CALL WORKSHEET (51-01-07)
- 1995-12-01: NEW PROCEDURE FOR ORDERING SERVICE REPL. EE PROMS (34-02-02)
- 1995-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE (53-65-07)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-10-09: INFO. ON DAYTIME RUNNING LAMPS (DRL) (53-82-09)
- 1995-09-01: WARRANTY INFORMATION - LABOR TIME SUBMISSION FORMAT (58-05-01A)
- 1995-09-01: REPLACEMENT OF ISOLATION DIODES (93-8-20)
- 1995-08-10: REVISED TECH 1 MASS STORAGE CARTRIDGE (MSC) OXYGEN SENSOR (51-65-47)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-06-01: CAMPAIGN: FRONT SHOULDER BELT SEW STOP STUCK IN RETRACTOR (90-C-53)
- 1995-06-01: CAMPAIGN: FRONT SHOULDER BELT SEW STOP STUCK IN RETRACTOR (5D22)
- 1995-05-23: WARRANTY ADMINISTRATION WARRANTY INFORMATION (57-05-02)
- 1995-05-15: INFORMATION ON CONTAMINATED R12 REFRIGERANT TESTING (53-12-05)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-28: WARRANTY ADMINISTRATION DEALER/RETAILER ADMINISTRATION (57-05-01)
- 1995-03-01: SMU - SECTION 0 - GENERAL INFORMATION (57-02-01)
- 1995-02-21: SMU - SECTION 6A - REVISED BALANCE SHAFT (57-61-07)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-01-11: ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-10)
- 1994-12-01: WEBESTO SUNROOF REPAIRS (81-15-26)
- 1994-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-07)
- 1994-11-23: FRONT BRAKE PULSATION - 'NEW' DIAGNOSIS (43-50-09)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-08-03: WARRANTY ADMINISTRATION-NEW WARRANTY CLAIM PROCESSING SYS. (41-05-02)
- 1994-07-22: INFORMATION ON DIAGNOSING SIR DTC 24 ALL DERM SYSTEMS (44-90-01)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-06-30: INFORMATION ON J39400 A/C LEAK DETECTOR MAINTENANCE KIT (43-12-18A)
- 1994-06-20: INFORMATION ON SPEED RATED TIRES (43-35-02)
- 1994-06-08: WARRANTY ADMINISTRATION - NEW LABOR OPERATION NUMBER (42-05-06)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-05-01: INFO. ON VEHICLES EQUIPPED WITH A WEBASTO SUNROOF (43-10-18A)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-15: INFORMATION ON TRANSAXLE OIL FILTER DIFFERENCES (47-71-03)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1994-01-26: WARRANTY ADMINISTRATION RECYCLED ENGINE COOLANT POLICY (31-05-04)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-12-07: NEW DCS BULN. SEARCH & ACCESS TO VEH. OPTION CONTENT RECORDS (33-01-06A)
- 1993-10-22: CLEARCOAT DEGRADATION-CHALKING & WHITENING (REPAIR PROCEDURE) (33-17-08)
- 1993-08-30: BCM EPROM CALIBRATIONS SUMMARY OF SERVICE EPROMS (93-8C-130)
- 1993-08-26: INTERMIT. PULL W/O HARD BRAKE APPLY DURING NON-ABS STOP (31-50-04)
- 1993-08-01: TIRES SLIPPING ON WHEELS USE PROPER TIRE MOUNTING PROC (93-3-6)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-3-10)
- 1993-08-01: TIRES SLIPPING ON WHEELS USE PROPER TIRE MOUNTING PROC (93-3E-103)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-3E-104)
- 1993-07-26: COLD START STALL-CHUGGLE AT 35-45 MPH WITH TCC (91-638-111)
- 1993-07-08: SERVICE MANUAL UPDATE-SEC 3F5A (SIR) TILT COLUMN UNIT REPAIR (93-3-15)
- 1993-07-08: SERVICE MANUAL UPDATE-SEC 3F5A (SIR) TILT COLUMN UNIT REPAIR (93-3B-602)
- 1993-07-01: LEAKING CAST ALUMINUM WHEELS (REPAIR WITH ADHESIVE SEALANT) (93-3-14)
- 1993-06-15: AIR CONDITIONING COMPRESSOR REPLACEMENT (NEW PROCEDURE) (93-1B-124)
- 1993-05-31: HORN CHIRPS INTERMITTENTLY (INSTALL NEWTON CONTACT ASSY.) (93-8A-119)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-0-6)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7-1)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-142)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1-9)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-05-01: RETURN OF UNDEPLOYED (SIR) INFLATOR MODULES (92-9-3)
- 1993-04-30: NEW TOOL FOR OPTICAL REDUNDANT STEERING WHEEL CONTROL SYSTEM (93-8A-632)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-04-05: CRANK (OR NO CRANK) AND NO START AND/OR NO START (31-81-13)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-03-01: SMU - SEC. 6E3, 6E2 DRIVEABILITY AND EMISSIONS (93-6E-14)
- 1993-03-01: SMU - SEC. 6E3, 6E2 DRIVEABILITY AND EMISSIONS (93-6E-121)
- 1993-02-27: A/C COMPRESSOR MOAN NOISE RPL.A/C COMP. CLUTCH DRIVER (93-1D-101)
- 1993-02-27: ENGINE STALLS ON COAST DOWN CLEAN CARBON DEPOSITS (93-6E-114)
- 1993-02-15: INTERMITTENT CODES E047,B333 B334,B335,B336 AND/OR B337 (93-8A-110)
- 1993-01-30: SERVICE PROCEDURE - CODE E39 VISCOUS CONVERTER CLUTCH DIAG. (93-7A-117)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1992-12-15: INOPERATIVE POWER MODULE REPLACEMENT (CHECK PROCEDURE) (93-1B-105)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: IMPROPER AIR DELIVERY FROM ECC (SERVICE INFORMATION/PROC.) (93-1A-101)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (92-6E-23)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (93-6C-100)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-14: DECEL STALL/CRANK ON START UP (NEW IAC MOTOR) (93-6E-102)
- 1992-11-14: TRANS. CONTROL LEVER SHIFTERS EFFORT (REPLACE LEVER) (93-7A-107)
- 1992-11-04: SERV. MAN UPDATE-SECTION 9J-A DIAG. OF INTERMIT. SIR CODE 24 (93-8-2)
- 1992-11-04: SERV. MAN UPDATE-SECTION 9J-A DIAG. OF INTERMIT. SIR CODE 24 (93-9-604)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-7)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-179)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-10-01: DECEL STALL/CRANK ON START UP - NEW IAC MOTOR (93-6E-3)
- 1992-10-01: SIR SYSTEM DIAG. ENERGY RESERV MODULE EXCHANGE (93-10-3)
- 1992-08-03: ALTERNATE REFRIGERANTS INFORMATION (92-1-16)
- 1992-07-01: COLD START STALL-CHUGGLE AT 35-45 MPH WITH TCC (91-6E-21A)
- 1992-06-22: CAMPAIGN: REAR BUMPER DURAB. AND APPEARANCE AND NOISE (91-C-6)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-17)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-123)
- 1992-06-15: ENGINE STALLS ON COAST DOWN CLEAN CARBON DEPOSITS (91-649-103)
- 1992-06-15: INTERMITTENT NO CRANK (REPLACE STARTER ENABLE RELAY) (92-8-150)
- 1992-06-01: LEAD OR PULL TO THE LEFT INSTALL SHIMS OR LEFT MOUNT (92-3-15)
- 1992-06-01: LEAD OR PULL TO THE LEFT INSTALL SHIMS OR LEFT MOUNT (92-3-125)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-1-13)
- 1992-04-30: INTERMITTENT NO CRANK (REPLACE STARTER ENABLE RELAY) (92-8-24)
- 1992-04-30: PWR. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (90-3-142)
- 1992-04-07: INSIDE DOOR HANDLE PULLS LOOSE REPLACE PULL HANDLE INSERT (91-10-43)
- 1992-04-07: INSIDE DOOR HANDLE PULLS LOOSE REPLACE PULL HANDLE INSERT (91-2-284)
- 1992-04-01: PROM I.D. NOT RECOGNIZED BY THE T-100 (GM CAMS) TERMINAL (23-65-08)
- 1992-03-25: TECH-1 GM 88-92 BRAKE CARTRIDGE EXCHANGE PROGRAM (92-1-12)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-12)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1992-03-24: KEYLESS ENTRY PERFORMANCE DIAGNOSIS/REPLACE TRANSMITTER (93-9-117)
- 1992-03-02: ENG. OIL LEAK - REAR MAIN SEAL (NEW REAR MAIN SEAL RELEASED) (92-6-8)
- 1992-03-02: ENG. OIL LEAK - REAR MAIN SEAL (NEW REAR MAIN SEAL RELEASED) (92-638-104)
- 1992-02-21: HUB ASSY. SEAL SQUEAK/SQUAWK NOISE (LUBE SEAL & HUB ASSY.) (91-3-21)
- 1992-02-21: HUB ASSY. SEAL SQUEAK/SQUAWK NOISE (LUBE SEAL & HUB ASSY.) (91-3-138)
- 1992-02-05: CRUISE CONTROL DROPOUT (FAILS TO SET OR RESUME) (92-9-9)
- 1992-02-05: CRUISE CONTROL DROPOUT (FAILS TO SET OR RESUME) (92-8-140)
- 1992-01-31: A/C R-12 CHARGING CAPACITY (CHART) (92-1-109)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-74T60-5)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-74T60-104)
- 1992-01-09: SIR SENSOR REPLACE POLICY REV. ALL 1988-92 CARS WITH SIR (92-9-8)
- 1992-01-09: SIR SENSOR REPLACE POLICY REV. ALL 1988-92 CARS WITH SIR (92-8-127)
- 1991-12-20: CONVERTIBLE SHAKE/JITTER (PROCEDURE TO IMPROVE) (91-10-40)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-4)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-103)
- 1991-12-14: ENGINE STALL ON COAST DOWN PERFORM DIAG. AND CLEAN CARBON (92-649-100)
- 1991-12-13: CAMPAIGN: BRAKE SYS. INDICATOR LIGHT INOPERABLE (1D22)
- 1991-12-02: ENGINE OIL LIFE INDEX RESET PROCEDURES AND INFORMATION (93-8C-119)
- 1991-11-30: ENGINE OIL ECONOMY (INFORMATIONAL BULLETIN) (93-6A-124)
- 1991-11-20: CAMPAIGN: BRAKE SYSTEM LAMP (REPLACE PROM IN BCM) (90-C-12)
- 1991-11-15: INTERMITTENT NO START/NO CRANK DUE TO PASSKEY (REPLACE KEY) (92-8-111)
- 1991-11-15: A/C R-12 CHARGING CAPACITY CADILLAC CHARGING TABLE (92-8-112)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-10-20)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-2-141)
- 1991-10-15: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1-2)
- 1991-10-11: A/C COMPRESSOR SEALING WASHER USAGE (NEW DESIGN) (92-1-3)
- 1991-10-11: A/C COMPRESSOR SEALING WASHER USAGE (NEW DESIGN) (92-1-103)
- 1991-10-03: HUM/WHINE NOISE FROM FRONT OF ENGINE-INSTALL NEW FRT. COVER (91-6-8)
- 1991-10-03: HUM/WHINE NOISE FROM FRONT OF ENGINE-INSTALL NEW FRT. COVER (91-638-112)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-2)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-100)
- 1991-09-30: SIR DIAGNOSTIC RESERVE MODULE (DERM) EXCHANGE PROGRAM (93-9-102)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-09-20: BINDING AT DOOR GUIDE PINS REPLACE DOOR PIN/LOCATOR ASSY. (90-10-45)
- 1991-09-20: BINDING AT DOOR GUIDE PINS REPLACE DOOR PIN/LOCATOR ASSY. (90-2-271)
- 1991-09-14: ENGINE STALLS ON COAST DOWN (CLEAN CARBON DEPOSITS) (90-645-118)
- 1991-09-10: CAUTIONS REGARDING SIR SYSTEM REPAIRS AND PROCEDURES (92-10-7)
- 1991-09-10: CAUTIONS REGARDING SIR SYSTEM REPAIRS AND PROCEDURES (92-8-106)
- 1991-08-28: SERVICE GUILD: ENGINE OIL LEAK AT REAR MAIN SEAL (90-6-14)
- 1991-08-28: SERVICE GUILD: ENGINE OIL LEAK AT REAR MAIN SEAL (90-6-119)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-4T60-3)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-74T60-100)
- 1991-08-15: ANTI-LOCK BRAKE PEDAL SQUEAK (INSTALL NEW SHIM) (90-5-132)
- 1991-08-15: FLASHING TELLTALES/IPC DISPLAY WITH IGNITION OFF (NEW PART) (91-8-232)
- 1991-08-13: PROPER PROC. FOR PROBING WIRES (NEW TEST PROBES AVAILABLE) (91-8-33)
- 1991-08-09: CELLULAR TELEPHONE PROGRAM (DELCO ELECT.) NEW INFORMATION (92-9-4)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-3)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-115)
- 1991-08-06: OIL PRESSURE GAGE ERRATIC (REPLACE OIL PRESS. SENSOR) (90-6D-6)
- 1991-08-06: OIL PRESSURE GAGE ERRATIC (REPLACE OIL PRESS. SENSOR) (92-8-103)
- 1991-07-31: 50-55 MPH SHAKE ON SMOOTH ROAD (REPLACE CRADLE MOUNTS) (91-2-230)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (92-6E-3)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-07-15: UNWANTED BLOWER OPERATION OR IMPROPER AIR DELIVERY ECC (91-1-138)
- 1991-07-12: SERVICE MANUAL UPDATE SEC. 7A TRANSAXLE REMOVAL/INSTALLATION (90-7-5)
- 1991-07-12: SERVICE MANUAL UPDATE SEC. 7A TRANSAXLE REMOVAL/INSTALLATION (90-7A-001)
- 1991-07-12: H/LAMP ACTUATOR CONTROL MODULE PARTS SYSTEM ERROR (NEW P/N) (91-8-230)
- 1991-06-29: REVISED OIL PAN GASKET CONTAINS CIRCULAR SPACERS (90-645-119)
- 1991-06-29: ECC SYSTEM CONTROLS TOO COLD (REPLACE BCM PROM) (91-1-133)
- 1991-06-20: DISPOSAL OF LIVE (UNDEPLOYED) SIR INFLATOR MODULES (92-9-2)
- 1991-06-13: RETAINING MEMORIES IN ELECT. DEVICES WITH BAT. DISCONNECTED (91-8-212)
- 1991-05-30: POWER ANTENNA MAY NOT RETRACT SEND RADIO TO DELCO FOR REPAIR (90-9-6)
- 1991-05-30: ERRATIC ECC MODE CHANGE INSPECT VACUUM HOSE (91-1-11)
- 1991-05-30: SERVICE MANUAL UPDATE REVISED FLYWHEEL TORQUE SPECS (91-6A-10)
- 1991-05-30: POWER ANTENNA MAY NOT RETRACT SEND RADIO TO DELCO FOR REPAIR (90-8-271)
- 1991-05-30: ERRATIC ECC MODE CHANGE INSPECT VACUUM HOSE (91-8-208)
- 1991-05-30: SERVICE MANUAL UPDATE REVISED FLYWHEEL TORQUE SPECS (91-6A-003)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISSING ACCESS CAPS (91-1-4)
- 1991-04-30: SIR SYSTEM DIAGNOSTIC ENERGY RESERVE MODULE(DERM) EXCHANGE (91-2-124)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-22: FRONT HEADER WAVINESS CLEAN UPPER SURFACE/UNDERSIDE (90-10-44)
- 1991-04-22: FRONT HEADER WAVINESS CLEAN UPPER SURFACE/UNDERSIDE (91-2-210)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6E-18)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6-117)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-0-5)
- 1991-04-15: LOW OIL LEVEL MESSAGE OPERATION-NEW SENSOR RELEASED (91-8-183)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-2-197)
- 1991-04-10: NEW DESIGN SPARK PLUG SERVICE INFORMATION (91-6E-15)
- 1991-04-10: NEW DESIGN SPARK PLUG SERVICE INFORMATION (91-638-110)
- 1991-04-05: CAMPAIGN: INFLATOR MODULE S.I.R. INFORMATION (90-C-9A)
- 1991-03-31: CAMPAIGN: SIR INFLATOR MODULE SEPARATION (INSPECT/REPLACE) (0A25A)
- 1991-02-28: SER. REPLACEMENT VALVE SPRING AND CAP ASSY. RELEASED (91-633-101)
- 1991-02-28: TIRE DAMAGE CAUSED IN GM ASSY. PLANTS-REPLACEMENT PROCEDURES (91-3-115)
- 1991-02-27: WIPER STARTS IN HIGH SPEED ONLY-REPLACE PARK SWITCH ASSY. (90-8-23)
- 1991-02-27: WIPER STARTS IN HIGH SPEED ONLY-REPLACE PARK SWITCH ASSY. (90-8-267)
- 1991-02-25: SERVICE INFO MANUAL REVISION SIR SYSTEM DIAGNOSIS (90-8-266)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-6D-5)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (91-6-111)
- 1991-02-15: COMPUTER COMMAND RIDE (CCR) SPEED DEPENDENT SYSTEM UPDATE (91-8-157)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1991-01-31: SHOULDER BELT CONTACTS NECK OF DRIVER AND FRONT PASSENGER (91-2-130)
- 1991-01-23: INSTALLATION & SEATING OF THE SIR COIL ASSY. (91-3-5)
- 1991-01-23: INSTALLATION & SEATING OF THE SIR COIL ASSY. (91-8-160)
- 1991-01-15: WATER LEAK/WIND NOISE AT TOP OF STATIONARY VENT GLASS (90-10-39)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-633-103)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-638-104)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-73T40-101)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-74T60105)
- 1991-01-15: SIR SYSTEM DIAGNOSTIC ENERGY RESERVE MODULE EXCHANGE (DERM) (91-8-125)
- 1991-01-14: SER. REPLACEMENT VALVE SPRING AND CAP (NEW SERVICE KIT) (91-6-5)
- 1991-01-14: SER. REPLACEMENT VALVE SPRING AND CAP (NEW SERVICE KIT) (91-638-108)
- 1991-01-02: SERVICE MANUAL UPDATE SEC.8D1 ECM TROUBLE CODE DIAGNOSIS (90-8-22)
- 1991-01-02: SERVICE MANUAL UPDATE SEC.8D1 ECM TROUBLE CODE DIAGNOSIS (90-638-111)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-0-4)
- 1990-12-31: SUPPLEMENTAL INFLATABLE RESTRAINT (INFLATOR MODULE) (90-C-9)
- 1990-12-31: ENGINE OIL LEAK AT THE OIL PAN (INSTALL NEW PAN/GASKET PKG.) (90-138-109)
- 1990-12-31: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (90-74T60123)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-2-123)
- 1990-12-31: BRAKE EFFECTIVENESS AFTER ROTOR REFINISHING (91-5-109)
- 1990-12-23: CAMPAIGN: SIR INFLATOR MODULE MAY SEPARATE FROM STG. WHEEL (0A25)
- 1990-12-15: NEW PLATES-4TH CLUTCH REACTION FORWARD CLUTCH/LOW & REV. (90-74T60-122)
- 1990-12-15: GRINDING OR GROWLING NOISE IN PARK ON INCLINE (90-74T60121)
- 1990-12-15: BCM EPROM CALIBRATIONS(SUMMARYOF SERVICE EPROM'S) (90-8-241)
- 1990-12-10: CLUTCH PLATE IDENTIFIERS FOR 3RD CLUTCH PLATE (91-74T60-7)
- 1990-12-10: SERVICE MANUAL UPDATE SEC.8A-4 SPECIFIC CURRENT DRAIN INFO (91-8-22)
- 1990-12-10: CLUTCH PLATE IDENTIFIERS FOR 3RD CLUTCH PLATE (91-74T60-116)
- 1990-12-10: SERVICE MANUAL UPDATE SEC.8A-4 SPECIFIC CURRENT DRAIN INFO (91-8-141)
- 1990-11-30: NO REVERSE/SLIPPING IN REVERSE REPEAT REVERSE BAND DISTRESS (90-74T60-120)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-8)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-114)
- 1990-11-21: LOW OIL LEVEL MESSAGE OPERATION/DIAG. & NEW PART (90-8-13)
- 1990-11-15: LOW OIL LEVEL MESSAGE NORMAL OPERATION (91-6D-2)
- 1990-11-15: ENGINE MISS ABOVE 3500 RPM'S MAY BE BROKEN CAMSHAFT LOBE (90-638-108)
- 1990-11-15: #4 REAR MAIN BEARING CAP PROC. FOR REMOVAL/INSTALLATION (91-638-100)
- 1990-11-15: LOW OIL LEVEL MESSAGE NORMAL OPERATION (91-8-134)
- 1990-11-14: SHOULDER BELT CONTACTS NECK OFDRIVER & PASSENGER (91-10-11)
- 1990-11-14: SERVICE MANUAL UPDATE SEC. 6 NEW BEARING CLEARANCE (91-6-4)
- 1990-11-14: SHOULDER BELT CONTACTS NECK OFDRIVER & PASSENGER (90-2-251)
- 1990-11-14: SERVICE MANUAL UPDATE SEC. 6 NEW BEARING CLEARANCE (91-630-101)
- 1990-10-31: CAMPAIGN: TRANS SHIFT CONTROL CABLE DISENGAGEMENT (0A32)
- 1990-10-25: ENGINE OIL LEAK AT OIL PAN (PAN & GASKET PKG.) (90-6-12)
- 1990-10-25: ENGINE OIL LEAK AT OIL PAN (PAN & GASKET PKG.) (90-633-109)
- 1990-10-25: DAY TIME RUNNING LIGHT MODULE PREVENTION OF FAILURES (91-8-120)
- 1990-10-15: CODE B446, B447 & B448 DIAG. REPLACE WITH REVISED PROM (90-1-133)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-15)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-108)
- 1990-10-08: INFO/RECOMMENDED FUELS FOR NON-TURBO PFI ENGINES (91-6E-3)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-7440-5)
- 1990-10-08: INFO/RECOMMENDED FUELS FOR NON-TURBO PFI ENGINES (91-6-103)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-74T60-109)
- 1990-09-30: CAMPAIGN: TRANSAXLE SHIFT CONTROL CABLE DISENGAGEMENT (90-C-7)
- 1990-09-30: SUPPLEMENTAL INFLATABLE RESTRAINT(DERM)EXCHANGE (91-10-2)
- 1990-09-27: LOOSE PULL STRAP ON DOOR TRIM (INSTALL NEW SHEET METAL CLIP) (90-10-38)
- 1990-09-27: LOOSE PULL STRAP ON DOOR TRIM (INSTALL NEW SHEET METAL CLIP) (90-2-242)
- 1990-09-21: AIR AND/OR WATER LEAK AT TOP OF DOOR GLASS TO VENT GLASS (91-10-7)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-7-1)
- 1990-09-21: AIR AND/OR WATER LEAK AT TOP OF DOOR GLASS TO VENT GLASS (91-2-112)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-74T60-106)
- 1990-09-15: NOISE FROM STEERING COLUMN NEAR INTERMEDIATE SHAFT (90-3-134)
- 1990-09-11: CONVERTIBLE TOP, DIFFICULT TO LATCH IN THE REAR (90-10-36)
- 1990-09-11: NO REVERSE/SLIPPING IN REVERSE REPEAT REVERSE BAND DISTRESS (91-7440-3)
- 1990-09-11: CONVERTIBLE TOP, DIFFICULT TO LATCH IN THE REAR (90-2-235)
- 1990-09-11: NO REVERSE/SLIPPING IN REVERSE REPEAT REVERSE BAND DISTRESS (91-74T60-104)
- 1990-09-10: DOORS ARE HARD TO OPEN CONVERTIBLE MODELS (91-10-3)
- 1990-09-10: DOORS ARE HARD TO OPEN CONVERTIBLE MODELS (91-2-109)
- 1990-09-07: QUARTER TRIMLOOSE FIT ALONG BACKLITE & SAIL AREA (90-10-33)
- 1990-09-07: SEAT SWITCH PLATES LOOSE REPLACE COVER & SCREWS (90-10-35)
- 1990-09-07: SEAT SWITCH PLATES LOOSE REPLACE COVER & SCREWS (90-2-236)
- 1990-09-07: QUARTER TRIMLOOSE FIT ALONG BACKLITE & SAIL AREA (90-2-237)
- 1990-08-31: BELT CHIRP OR SQUEAL SERVICE PROCEDURE (90-638-106)
- 1990-08-22: ENGINE MISS ABOVE 3500 RPM'S MAY BE BROKEN CAMSHAFT LOBE (90-6-8)
- 1990-08-22: ENGINE MISS ABOVE 3500 RPM'S MAY BE BROKEN CAMSHAFT LOBE (90-633-107)
- 1990-08-21: #4 REAR MAIN BEARING CAP R/R PROCEDURE OUTLINED (91-6-1)
- 1990-08-21: #4 REAR MAIN BEARING CAP R/R PROCEDURE OUTLINED (91-633-100)
- 1990-08-15: STATE EMISSIONS TESTING INFORMATION / PROCEDURE (91-6E-2)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-13)
- 1990-08-14: RADIO DISTORTION AT HIGH VOLUME FROM DOOR SPEAKERS (90-8-211)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-101)
- 1990-08-02: NEW WARRANTY CLAIM FAILURE CODES (90-0-10)
- 1990-07-31: VINYL TOP SCREW INTERFERENCE REMOVE POINT END OF SCREW (90-10-26A)
- 1990-07-26: RELEASE OF ANTENNA BEZEL NUT-1991 ESSENTIAL TOOL (91-9-3)
- 1990-07-24: BRAKE EFFECTIVENESS CHANGE AFTER ROTOR & BRAKE PAD WORK (90-5-12)
- 1990-07-18: SERVICE MANUAL UPDATE-SEC. 8D1 REVISED CODE E042 DIAG. CHART (90-8-15)
- 1990-07-18: SERVICE MANUAL UPDATE-SEC. 8D1 REVISED CODE E042 DIAG. CHART (90-638-107)
- 1990-07-13: WATER LEAK AND/OR WIND NOISE TOP OF STATIONARY VENT GLASS (90-2-208)
- 1990-07-09: SUN VISOR CLIPS RETENTION (REPLACE SUN VISOR CLIP) (90-10-42)
- 1990-07-09: NOISE FROM STEERING COLUMN NEAR INTERMEDIATE SHAFT (90-3-19)
- 1990-07-09: NOISE FROM STEERING COLUMN NEAR INTERMEDIATE SHAFT (90-2-205)
- 1990-07-09: SUN VISOR CLIPS RETENTION (REPLACE SUN VISOR CLIP) (90-2-206)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (91-3-1)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (90-3-127)
- 1990-06-28: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (90-6-7)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-10)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-118)
- 1990-06-15: FLOOR PAN OIL CANNING INSTALL BETA BRACE MATERIAL (90-10-30)
- 1990-06-15: FLOOR PAN OIL CANNING INSTALL BETA BRACE MATERIAL (90-2-203)
- 1990-06-08: RATTLE TYPE NOISE FROM REAR OF ENGINE - NEW DAMPENER P/N (90-6-6)
- 1990-06-08: RATTLE TYPE NOISE FROM REAR OF ENGINE - NEW DAMPENER P/N (90-638-105)
- 1990-05-24: REMOTE KEYLESS ENTRY RANGE OPERATION & SYSTEM FEATURES (90-9-4)
- 1990-05-24: REMOTE KEYLESS ENTRY RANGE OPERATION & SYSTEM FEATURES (90-8-203)
- 1990-05-23: REAR ROOF PIN ALIGNMENT AND LOCK LATCH CABLE ADJUSTMENTS (90-10-28)
- 1990-05-23: REAR ROOF PIN ALIGNMENT AND LOCK LATCH CABLE ADJUSTMENTS (90-2-186)
- 1990-05-22: VINYL TOP SCREW INTERFERENCE REMOVE POINT END OF SCREW (90-10-26)
- 1990-05-22: STOWAGE PANEL HINGE DAMAGE MODIFY STOWAGE BOLT STUD (90-10-27)
- 1990-05-22: VINYL TOP SCREW INTERFERENCE REMOVE POINT END OF SCREW (90-2-184)
- 1990-05-22: STOWAGE PANEL HINGE DAMAGE MODIFY STOWAGE BOLT STUD (90-2-185)
- 1990-05-16: 1990 REATTA PORTFOLIO REATTA PEN, TIRE GAUGE, LIGHT (90-0-4)
- 1990-05-02: WHITE OVERSPRAY CONDITION CAUSE & POSSIBLE CORRECTION (03-17-02)
- 1990-05-02: SERVICE REPLACEMENT TRANS. (SRTA) ASSEMBLY MODEL UPDATE (90-7440-117)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-12)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-119)
- 1990-04-26: TRANSAXLE BOTTOM PAN LEAK(440) APPLYING SEALANT TO PAN BOLT (91-7440-2)
- 1990-04-26: TRANSAXLE BOTTOM PAN LEAK(440) APPLYING SEALANT TO PAN BOLT (90-7440-116)
- 1990-04-26: SERVICE MANUAL UPDATE-SEC. 8D DIAG. PHONE MODE DISPLAY BD45 (90-8-187)
- 1990-04-18: 4T60/440T4/F-7 CODES FOR NEW CHANNEL PLATE & INPUT HOUSING (90-7440-13)
- 1990-04-18: 4T60/440T4/F-7 CODES FOR NEW CHANNEL PLATE & INPUT HOUSING (90-7440-115)
- 1990-04-11: NEW OUTPUT SHAFT/BEARING & 3RD ROLLER CLUTCH ASSEMBLY (90-7440-10)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-7440-11)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (91-9-1)
- 1990-04-11: NEW OUTPUT SHAFT/BEARING & 3RD ROLLER CLUTCH ASSEMBLY (90-7440-113)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-7440-114)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-8-184)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (91-6B-1)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (90-6-107)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-6D-2)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-03-21: INSTALL CROSS CAB ENGINE COMPARTMENT STRUT TOWER BRACE (90-2-162)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-8)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-112)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6E-15)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6-105)
- 1990-02-27: SERVICE INFO. & PACKAGES DISTRESSED 4TH CLUTCH (90-7440-6)
- 1990-02-27: SERVICE INFO. & PACKAGES DISTRESSED 4TH CLUTCH (90-7440-110)
- 1990-02-17: CAMPAIGN: REAR SHOULDER BELT PENDULUM INTERFERENCE (90-C-3)
- 1990-02-17: CAMPAIGN: REAR SHOULDER BELT PENDULUM INTERFERENCE (0A09)
- 1990-02-16: CAMPAIGN: SUPPLEMENTAL INFLATABLE RESTRAINT SENSOR (90-C-1)
- 1990-02-16: CAMPAIGN: SUPPLEMENTAL INFLATABLE RESTRAINT SENSOR (0A10)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-9)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-111)
- 1990-02-13: A/C R-12 SERVICE PROCEDURES CHARGING CAPACITY CHART (90-1-119)
- 1990-02-10: SUPPLEMENTAL INFLATABLE RESTRAINT (SIR) DERM EXCHANGE (90-8-139)
- 1990-02-02: STEERING WHEEL REMOVAL VEH. W/SIR OR REDUNDANT S.W.C. (90-9-1)
- 1990-02-02: SERVICE MANUAL UPDATE SEC. 8A-INSTRUMENT PANEL (90-8-8)
- 1990-02-02: STEERING WHEEL REMOVAL VEH. W/SIR OR REDUNDANT S.W.C. (90-2-138)
- 1990-02-02: SERVICE MANUAL UPDATE SEC. 8A-INSTRUMENT PANEL (90-8-141)
- 1990-01-30: ELECTRONIC INSTR. CLUSTER EXCHANGE/REPAIR PROGRAM (90-8-6)
- 1990-01-16: INOPERATIVE CRUISE CONTROL (REPLACE VACUUM HOSE) (90-8-134)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-7A)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-109)
- 1989-12-22: TWILIGHT SENTINEL POTENTIOMETER LED MISSING (90-8-4)
- 1989-12-22: TWILIGHT SENTINEL POTENTIOMETER LED MISSING (90-8-126)
- 1989-12-08: INSTRUMENT CLUSTER EXCHANGE REPAIR PROGRAM (90-8-124)
- 1989-12-06: NEW WIRING HARNESS AND PRESSURE SWITCHES (90-7440-5)
- 1989-12-06: NEW WIRING HARNESS AND PRESSURE SWITCHES (90-7440-107)
- 1989-12-02: SUPPLE. INFLATABLE RESTRAINT SYS. WIRING REPAIR PROCEDURES (90-10-11)
- 1989-12-02: SUPPLE. INFLATABLE RESTRAINT SYS. WIRING REPAIR PROCEDURES (90-8-125)
- 1989-11-27: WATER LEAK AT PLENUM CHAMBER DRAIN COWL AREA (90-10-13)
- 1989-11-27: WATER LEAK AT PLENUM CHAMBER DRAIN COWL AREA (90-2-125)
- 1989-11-22: 1990 MODEL WHEEL ALIGNMENT SPECIFICATIONS (90-3-7)
- 1989-11-22: 1990 MODEL WHEEL ALIGNMENT SPECIFICATIONS (90-3-109)
- 1989-11-21: DOOR LOCK MODULE RATTLE (INSTALL NEW RIVET) (90-10-10A)
- 1989-11-21: DOOR LOCK MODULE RATTLE (INSTALL NEW RIVET) (90-2-120)
- 1989-11-17: EXTENDED CRANK TIME (NEW PART) (90-6E-8)
- 1989-11-17: EXTENDED CRANK TIME (NEW PART) (90-638-104)
- 1989-11-14: ASSEMBLY PLANT PAINT I.D. (90-10-7)
- 1989-11-14: ASSEMBLY PLANT PAINT I.D. (90-2-118)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-10-9)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-2-114)
- 1989-11-02: NEW DRIVEN SPROCKET SUPPORT AND CHAIN SCAVENGING SCOOP (90-7440-2)
- 1989-11-02: NEW DRIVEN SPROCKET SUPPORT AND CHAIN SCAVENGING SCOOP (90-7440-103)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7-3A)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7440-104)
- 1989-10-30: 3RD CLUTCH & OVERHAUL KITS MAY REQUIRE CALIBRATION UPDATE KIT (90-7440-3)
- 1989-10-30: INFORMATION ON NEW TWO PLATE 4TH CLUTCH ASSEMBLY (90-7440-4A)
- 1989-10-30: INFORMATION ON NEW TWO PLATE 4TH CLUTCH ASSEMBLY (90-7440-102)
- 1989-10-30: 3RD CLUTCH & OVERHAUL KITS MAY REQUIRE CALIBRATION UPDATE KIT (90-7440-106)
- 1989-10-27: NEW PARKING LOCK SYSTEM FOR HEAVIER GROSS VEHICLE WEIGHT (90-7440-1)
- 1989-10-27: NEW PARKING LOCK SYSTEM FOR HEAVIER GROSS VEHICLE WEIGHT (90-7440-105)
- 1989-10-23: 1990 FRENCH LABEL INSTALLATION INSTRUCTIONS (90-0-100)
- 1989-10-19: SLOW AIR LEAKS AT TIRE WHEEL WEIGHTS (PROCEDURE/NEW PART) (90-3-4)
- 1989-10-19: SLOW AIR LEAKS AT TIRE WHEEL WEIGHTS (PROCEDURE/NEW PART) (90-3-106)
- 1989-10-18: SEAT BELT COMFORT FEATURE ELIMINATED (90-10-1A)
- 1989-10-18: SEAT BELT COMFORT FEATURE ELIMINATED (89-2-186)
- 1989-10-13: SERVICE GUILD: SUPPLEMENTAL INFLATABLE (SIR) RESTRAINT (90-10-3)
- 1989-10-13: REVISED CYLINDER HEAD BOLT TORQUING PROCEDURE (90-6A-1A)
- 1989-10-13: CYLINDER HEAD BOLT TORQUING PROCEDURE (90-6A-1)
- 1989-10-13: REVISED CYLINDER HEAD BOLT TORQUING PROCEDURE (90-638-100)
- 1989-10-13: SERVICE GUILD: SUPPLEMENTAL INFLATABLE (SIR) RESTRAINT (90-8-113)
- 1989-10-11: 1990 NEW VEHICLE ANNOUNCEMENT BULLETIN INFORMATION (90-0-1)
- 1989-10-10: THEFT PREVENTION STANDARDS ANTI-THEFT LABELING (90-0-2)
- 1989-10-10: THEFT PREVENTION STANDARDS ANTI-THEFT LABELING (90-0-103)
- 1989-10-09: REVISED LTG FORMAT AUTO/MANUAL TRANSMISSION (90-7-2)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-8-114)
- 1989-10-06: TIRE COMPANY WARRANTY ASSISTANCE PROGRAMS (90-3-3)
- 1989-09-27: SERVICE GUILD: USE OF FUEL WITH 15% MTBE IN ALL GM VEH. (89-0-7)
- 1989-09-13: SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM (90-2-113)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-6B-1)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0-101)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-15)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-07-16: NEW REVERSE BAND APPLY PIN GAGE (89-7440-11)
- 1989-07-16: NEW REVERSE BAND APPLY PIN GAGE (90-7440-100)
- 1989-06-07: NEW TRANSAXLE I.D. CODES INFO. ON NEW OVERHAUL PACKAGES (89-7440-10)
- 1989-06-07: NEW TRANSAXLE I.D. CODES INFO. ON NEW OVERHAUL PACKAGES (89-7440-111)
- 1989-06-06: LOW OIL LEVEL MESSAGE OPERATION/DIAGNOSIS & NEW PART (90-8-160)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-8)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-110)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (90-6-5)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (89-6-115)
- 1989-01-14: ANTI-LOCK BRAKE PEDAL SQUEAK INSTALL SHIM (89-5-7)
- 1989-01-14: ANTI-LOCK BRAKE PEDAL SQUEAK INSTALL SHIM (89-5-106)
- 1988-08-10: TRI-COAT PAINT REPAIR PROCEDURES (93-10-115)
- 1988-02-04: ODOR FROM A/C AT START-UP PROCEDURE TO REPAIR DESCRIBED (90-1-1)
- 1987-11-16: DELCO BATTERY STORAGE TESTING DIAGNOSIS AND CHARGING (87-8-5)
- 1987-11-16: DELCO BATTERY STORAGE TESTING DIAGNOSIS AND CHARGING (89-8-109)