For 1990-2009 cars

### Removal Procedure

1. Remove the front end panel. Refer to Front End Panel Replacement .
2. Remove the screws retaining the diagonal braces to the front end panel.
3. Remove the brace from the snap-in holder.
4. Remove the brace.

### Installation Procedure

1. Install the brace in the snap-in holder.
2. Install the nuts in order to retain the diagonal braces to the front end panel.

Tighten
Tighten the bolts and the nut to 10.5 N·m (93 lb in).

3. Install the front end panel. Refer to Front End Panel Replacement .