For 1990-2009 cars

Important: Before entering the programming mode, verify possession of all the transmitters you will be using on the vehicle. Once you program the transmitter, the memory erases. The other transmitters will not be functional until you program the transmitters again. You may program up to 4 transmitters.

Perform the following procedure when adding new transmitters or replacing failed transmitters:

1. Turn OFF the ignition switch.
2. Use a fused jumper wire in order to jumper the Data Line Connector terminal 8 (BLK/WHT) to terminal 4 (BLK).
3. Close all of the doors.
4. Turn ON the ignition switch.

The doors will cycle to lock.

5. Press and hold the following buttons on one of the transmitters:

• | LOCK

• | UNLOCK

6. After a 30 second delay, the doors will lock and unlock.
7. In order to program extra transmitters, repeat Step 5.

Important: Do not turn off the ignition. If the switch is turned off, the first transmitter becomes inoperative.

8. Disconnect the fused jumper wire from the DLC.