For 1990-2009 cars

### Removal Procedure

1. Remove the case side cover. Refer to Control Valve Body Cover Replacement .
2. Use a small flat-bladed tool in order to remove the wiring harness from the solenoid valve(s) (315A, 315B, 322, 334 and/or 440), TFP manual valve position switch (395) and/or the temperature sensor (391).
3. Remove the wiring harness (224).
4. Remove the clips retaining the solenoid(s).
5. Remove the solenoid(s).
6. Remove the 2-3 shift solenoid (315B).
7. Inspect the wiring harness (224).

### Installation Procedure

1. Install the 2-3 shift solenoid (315B).
2. Install the solenoid(s).
3. Install the retaining clips.
4. Install the wiring harness (224).
5. Install the wiring harness to the solenoid valve(s) (315A, 315B, 322, 334 and/or 440), TFP manual valve position switch (395) and/or the temperature sensor (391).
6. Install the case side cover. Refer to Control Valve Body Cover Replacement .