For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment front trim. Refer to Rear Compartment Trim Panel Replacement .
2. Remove the rear compartment sill plate and the rear trim. Refer to Rear Compartment Sill Trim Plate Replacement .
3. Remove the rear compartment side trim. Refer to Rear Compartment Side Trim Replacement - Right Side .
4. Remove the spare tire cover.
5. Remove the spare tire.
6. Remove the jack.
7. Fold inward and lift out the rear compartment floor trim (1).

### Installation Procedure

1. Install the rear compartment floor trim (1) to the vehicle.
2. Feed the fuel door emergency release handle through the trim panel.
3. Install the jack.
4. Install the spare tire.
5. Install the spare tire cover.
6. Install the rear compartment side trim. Refer to Rear Compartment Side Trim Replacement - Right Side .
7. Install the rear compartment sill plate/rear trim. Refer to Rear Compartment Sill Trim Plate Replacement .
8. Install the rear compartment front trim. Refer to Rear Compartment Trim Panel Replacement .